For 1990-2009 cars

The following procedure describes how to inspect the wheel bearing/hub for excessive looseness. If you are inspecting the wheel bearing/hub for excessive runout, refer to Tire and Wheel Vibration in Vibration Diagnosis and Correction.

#### Tools Required

J 8001 Dial Indicator

Important: If you are inspecting the FRONT wheel bearing/hub, support the front of the vehicle by the lower control arms in order to load the lower ball joint.

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Mount and secure the J 8001 to a stand.
3. Ensure that the J 8001 contacts the vertical surface of the wheel as close as possible to the top wheel stud.
4. Push and pull on the TOP of the tire.
5. Inspect the total movement indicated by the J 8001 .
6. If the measurement exceeds 0.127 mm (0.005 in), replace the wheel bearing/hub. Refer to Front Wheel Bearing and Hub Replacement in Front Suspension or Rear Wheel Bearing and Hub Replacement in Rear Suspension.