For 1990-2009 cars

### Removal Procedure

1. Remove the video cassette player center console. Refer to Center Console - Video Cassette Player Replacement .
2. Cut the plastic tie strap and remove the video cassette player noise supression ring and wiring harness from the H-bracket.
3. Unwrap the wiring harness from the video cassette player noise supression ring.

### Installation Procedure

1. Wrap the video cassette wiring harness around the noise supression ring three times.
2. Wrap the noise supression ring with foam and route a new plastic tie strap through the foam and ring.
3. Secure the video cassette player noise supression ring to the H-bracket with the plastic tie strap.
4. Install the video cassette player center console. Refer to Center Console - Video Cassette Player Replacement .