For 1990-2009 cars

### Removal Procedure

#### Tools Required

J 42506 Door Handle Clip Remover

1. Use J 42506 in order to remove the door inside handle clip.
2. Remove the sliding door inside handle from the door.

### Installation Procedure

1. Load the door inside handle clip into the handle with the open end facing down.
2. Align the door inside handle with the shaft on the sliding door.
3. Press firmly in order to seat the sliding door inside handle.