For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 |

1. Use a test lamp in order to backprobe between B+ and the inoperative door lock switch connector terminal D.
2. Press the inoperative door lock switch to the UNLOCK position.

Does the test lamp light?

--

Go to Step 2

Go to Step 3

2 | Repair a poor connection or open in CKT 194. Is the repair complete? | -- | Go to Automatic Door Locks System Check | --
3 | Replace the door lock switch. Refer to Front Side Door Lock Replacement or Lock Replacement - Sliding Door Front in Doors. Is the repair complete? | -- | Go to Automatic Door Locks System Check | --