For 1990-2009 cars

### Removal Procedure

1. Remove the case side cover. Refer to Control Valve Body Cover Replacement .

Notice: Do NOT remove the three bolts which hold the pump together.

2. Remove the oil pump bolts (204-207).
3. Remove the oil pump (300).
4. For information on the disassembly and inspection of the oil pump. Refer to the Transmission/Transaxle/Transfer Case Unit Repair Manual.

### Installation Procedure

1. Install the oil pump (300) to valve body.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the oil pump bolts (204-207).

Tighten

• | Tighten the M6 bolt to 11 N·m (97 lb in).

• | Tighten the M8 bolt to 24 N·m (18 lb ft).

3. Install the case side cover. Refer to Control Valve Body Cover Replacement .