For 1990-2009 cars

### Removal Procedure

1. Disable the SIR system. Refer to Disabling the SIR System in SIR.
2. Remove the connector position assurance (CPA) from the inflatable restraint steering wheel module coil yellow 2-way connector at the base of the steering column.
3. Disconnect the inflatable restraint steering wheel module coil yellow 2-way connector.
4. Remove the upper and lower shrouds. Refer to Steering Column Shrouds - Disassemble.
5. Remove the inflatable restraint steering wheel module. Refer to Steering Wheel Inflator Module Replacement .
6. Remove the steering wheel. Refer to Steering Wheel Replacement .
7. Remove the wire harness straps from the steering wheel column wire harness.
8. Remove the retaining ring.
9. Remove the inflatable restraint steering wheel module coil from the steering shaft.

### Installation Procedure

1. Install the inflatable restraint steering wheel module coil to the steering shaft.
2. Install the retaining ring.
3. Route the lower coil wire harness along steering column jacket.
4. Install the wire harness straps to the steering wheel column wire harness.
5. Install the steering wheel. Refer to Steering Wheel Replacement .
6. Install the inflatable restraint steering wheel module. Refer to Steering Wheel Inflator Module Replacement .
7. Install the upper and lower shrouds. Refer to Steering Column Shrouds - Disassemble.
8. Connect the inflatable restraint steering wheel module yellow 2-way connector at the base of the steering column.
9. Install the CPA to the inflatable restraint steering wheel module coil yellow 2-way connector.
10. Enable the SIR system. Refer to Enabling the SIR System in SIR.