For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to

   Caution: To help avoid personal injury when a vehicle is on a hoist, provide additional support for the vehicle at the opposite end from which components are being removed. This will reduce the possibility of the vehicle falling off the hoist.

   in General Information.
2. Remove the oil pan. Refer to Oil Pan Replacement .
3. Remove the filter. Refer to Automatic Transmission Fluid Filter and Seal Replacement .
4. Remove the accumulator attaching bolts.
5. Remove the manual 2-1 band servo cover bolts.
6. Remove the accumulator.
7. Remove the manual 2-1 band servo cover.
8. Remove the manual 2-1 band servo.
9. To disassemble, inspect and service the accumulator and 2 - 1 manual servo, refer to Transmission/Transaxle/Transfer Case Unit Repair Manual.

### Installation Procedure

1. Install the manual 2-1 band servo.
2. Install the manual 2-1 band servo cover.
3. Install the manual 2-1 band servo cover bolts.

Tighten
Tighten the manual 2-1 band servo cover bolts to 24 N·m (17 lb ft). Refer to

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

in General Information.
4. Install the accumulator.
5. Install the accumulator attaching bolts.

Tighten
Tighten the accumulator attaching bolts to 11 N·m (97 lb in).

6. Install the filter seal if previously removed.
7. Install the filter. Refer to Automatic Transmission Fluid Filter and Seal Replacement .
8. Install the oil pan. Refer to Oil Pan Replacement .