For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Inspect the FRT PWR SCKT fuse. Is the FRT PWR SCKT fuse open? | -- | Go to Step 2 | Go to Step 3
2 | Repair short to ground in circuit 1940. Has the repair been made and the system rechecked? | -- | System OK | --
3 | Use a test light in order to backprobe between the front electric accessory plug housing terminal A and ground. Does the test lamp light? | -- | Go to Step 5 | Go to Step 4
4 | Repair the open in circuit 1940. Has the repair been made and the system rechecked? | -- | System OK | --
5 | Use a test light in order to backprobe between the front electric accessory plug housing terminal A and terminal B. Does the test lamp light? | -- | Go to Step 7 | Go to Step 6
6 | Repair a poor connection or open in circuit 150. Has the repair been made and the system rechecked? | -- | System OK | --
7 | Replace the front accessory plug housing. Refer to Floor Console Accessory Power Receptacle Replacement in Instrument Panel Gauges and Console. Has the repair been made and the system rechecked? | -- | System OK | --