For 1990-2009 cars

### Removal Procedure

1. Use a heat gun in order to heat the sliding door upper guards. Hold the heat gun 152 mm (6 in) from the surface. Use a circular motion to apply heat for about 30 seconds.
2. Use a flat-bladed tool in order to peel the sliding door upper and lower guards from the panel surface. Be careful not to damage the paint.
3. Use oil-free naphtha or alcohol in order to clean the body panel.

### Installation Procedure

1. Use a heat lamp or heat gun in order to warm the body panel to a minimum of 21°C (70°F).
2. Peel the backing from the front end of the sliding door upper and lower guards. Do not touch the adhesive backing.
3. Press the sliding door upper and lower guards onto the body while continuing to remove the backing.
4. Hand roll the sliding door upper and lower guards to the body in order to ensure proper adhesion.