For 1990-2009 cars

# Info - New Frame Insulator Remover/Installer Available

Subject: | Information -- New Frame Insulator Remover/Installer From Kent Moore

Models: | 1997-2000 Buick Park Avenue

| 1997-2002 Buick Century, Regal

| 2000-2001 Buick LeSabre

| 2002 Buick Rendezvous

| 2000 Cadillac DeVille, Seville

| 1997-2001 Chevrolet Venture

| 1997-2002 Chevrolet Lumina, Monte Carlo

| 2000-2002 Chevrolet Impala

| 1998-2002 Oldsmobile Intrigue

| 2001 Oldsmobile Aurora

| 1997-1998 Pontiac Trans Sport

| 1997-2002 Pontiac Grand Prix

| 1999-2001 Pontiac Montana

| 2000-2001 Pontiac Bonneville

| 2001-2002 Pontiac Aztek

This bulletin contains information regarding a new service tool Frame Insulator Remover/Installer J-45296 which is now available from Kent Moore.

This tool aids in the removal and installation of the frame lower front insulator.

### Tool Usage Procedure

Within SI2000, refer to the Frame and Underbody sub-section for the complete procedure for replacing the frame lower front insulator.

1. Install the J-45296 Frame Insulator Remover/Installer to the front frame lower insulator you are removing.
2. Using J-45296 Frame Insulator Remover/Installer, remove the front frame lower insulator from the frame.
3. Using J-45296 Frame Insulator Remover/Installer, install the front frame lower insulator to the front frame.