For 1990-2009 cars

### Installation Procedure

#### Tools Required

• | J 28467-B

• | J 28467-500

1. Disconnect the battery ground (negative) cable.
2. Remove the right side engine mount strut. Refer to Engine Mount Strut Replacement .
3. Install the J 28467-500 .
4. Install the spreader bar to the engine mount strut bracket.
5. Install the spreader bar to the engine right side engine lift hook.
6. Install the J 28467-6A .
7. Install the J 28467-7A to the engine left side engine lift hook.
8. Install the J 28467-34 .
9. Install the J 28467-6A .
10. Install the J 28467-8A to the spreader bar.
11. Install the J 28467-34 .
12. The engine support fixture upper portion installed.
13. Raise and support the vehicle. Refer to General Information.

Important: Ensure that the J 28467-500UPD utility straps do not contact the frame in order to provide clearance for the frame removal.

14. Install the J 28467-500UPD hook to the engine mount.
15. Install the J 28467-500UPD opposite end hook to the underbody rail.
16. Install the OTHER J 28467-500UPD hook to the transaxle.
17. Install the J 28467-500UPD opposite end hook to the underbody rail.
18. Tighten both of the J 28467-500UPD utility straps in order to prevent movement of the powertrain.

### Removal Procedure

1. Remove both of the J 28467-500UPD .
2. Lower the vehicle.
3. Remove the J 28467-34 .
4. Remove the J 28467-7A .
5. Remove the J 28467-6A .
6. Remove the J 28467-34 .
7. Remove the J 28467-8A .
8. Remove the J 28467-6A .
9. Remove the J 28467-500 .
10. Install the right side engine mount strut. Refer to Engine Mount Strut Replacement .
11. Connect the battery ground (negative) cable.