For 1990-2009 cars

### Removal Procedure

1. Remove the instrument panel. Refer to Instrument Panel Assembly Replacement .
2. Pull on the wiring harness (2) in order to release the retainers.
3. Remove the wiring harness (2).

### Installation Procedure

1. Align the wiring harness retainers.
2. Push in on the wiring harness (2) until the harness is secure.

Important: Ensure that the electrical connectors are routed correctly through the instrument panel.

3. Install the instrument panel. Refer to Instrument Panel Assembly Replacement .