For 1990-2009 cars

### Removal Procedure

1. Remove the electrical connector from the idle air control valve, and throttle position sensor.
2. Remove the idle air control valve (2) attaching screws.
3. Remove the idle air control valve.
4. Remove the idle air control valve O-ring.

### Installation Procedure

Notice: The IAC valve may be damaged if installed with the cone (pintle) extended more than 28 mm (1-1/8 in). Measure the distance that the valve is extended before installing a new valve. The distance from the idle air control valve motor housing to the end of the idle air control valve pintle should be less than 28 mm (1-1/8 in). Manually compress the pintle until the extension is less than 28 mm (1-1/8 in).

1. Install the new idle air control O-ring .
2. Install the idle air control valve in the intake manifold.
3. Install the idle air control valve (2) attaching screws.

Tighten
The idle air control valve attaching screws to 3.0N·m (27 lb in).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

4. Install the electrical connector to the idle air control valve, and throttle position sensor.
5. The PCM will reset the idle air control valve whenever the ignition switch is turned ON, then OFF. Turn the ignition switch ON, then OFF.
6. Start the engine and allow the engine to reach operating temperature.