For 1990-2009 cars

### Removal Procedure

1. Remove the transaxle. Refer to Automatic Transaxle.
2. Remove the flywheel. Refer to Engine Flywheel Replacement .
3. Remove the crankshaft rear oil seal. Refer to Crankshaft Rear Oil Seal Removal .

### Installation Procedure

1. Install the seal. Refer to Crankshaft Rear Oil Seal Installation .
2. Install the flywheel. Refer to Engine Flywheel Replacement .
3. Install the transaxle. Refer to Automatic Transaxle.