For 1990-2009 cars

#### Tools Required

J 36850 Assembly Lubricant (or equivalent)

1. Assemble the carrier/sun gear thrust bearing (698), the final drive sun gear (697) with the chamfered side toward the parking gear (696) into the differential/final drive carrier assembly (700).
2. Assemble the parking gear (696) onto the final drive sun gear shaft (689)
3. Assemble the final drive sun gear shaft/parking gear assembly (689/696) into the final drive sun gear (697).

Important: Apply J 36850 or equivalent to the parking gear side of the bearing (695).

4. Assemble the internal gear/parking gear thrust bearing (695) to the parking gear (696).
5. Install the differential/final drive carrier assembly into the case.