For 1990-2009 cars

### Removal Procedure

1. Turn the ignition OFF.

Important: Note the position of the wires and the wire looms before removing.

2. Remove the spark plug wire(s) from front spark plugs by twisting the boot 1/2 turn before removing the spark plug boot.
3. Remove the spark plug wire retaining clips from the engine.
4. Rotate the engine forward. Refer to Engine Mechanical.
5. Remove the spark plug wire(s) from the rear spark plug(s).
6. Remove the spark plug wire retaining clips from rear of the engine.
7. Remove the spark plug wire(s) from the ignition coil(s).
8. Remove the spark plug wire(s) from the engine.

Important: If replacing the spark plug wires, transfer any of the spark plug wire conduit or the spark plug wire retaining clips.

### Installation Procedure

1. Install the spark plug wire(s) to the engine.
2. Install the spark plug wire(s) to the ignition coil(s).
3. Install the spark plug wire(s) to the rear spark plug(s).
4. Install the spark plug wire retaining clips to rear of the engine.
5. Return engine to proper position. Refer to Engine Mechanical.
6. Install the spark plug wire(s) to the front spark plug(s).
7. Install the spark plug wire retaining clips to front of the engine.