For 1990-2009 cars

### Removal Procedure

#### Tools Required

• | J 37609-A Power Steering Pump Pulley Remover

• | J 25033-C Power Steering Pump Pulley Installer or J 36015 Power Steering Pump Pulley Installer

1. Remove the drive belt. Refer to Drive Belt Replacement in Engine Mechanical - 3.4L.
2. Remove the power steering hoses from the power steering hose retainers.

Important: Do NOT disconnect the power steering hoses from the power steering pump.

3. Remove the power steering pump from the engine for clearance. Refer to Power Steering Pump Replacement .
4. Use the J 37609-A in order to remove the pump pulley.

### Installation Procedure

Important:

• | Ensure that the face of the pulley hub is flush with the end of the pump shaft.

• | Do not use the arbor press to install the pulley.

1. Use the J 25034-C or the J 36015 in order to install the power steering pump pulley.
2. Install the power steering pump to the engine. Refer to Power Steering Pump Replacement .
3. Install the drive belt. Refer to Drive Belt Replacement in Engine Mechanical - 3.4L.
4. Bleed the power steering system if the pump was removed. Refer to Power Steering System Bleeding .
5. Inspect the system for leaks. Refer to Power Steering System Test .