For 1990-2009 cars

#### Tools Required

J 23653-SIR Lock Plate Compressor

1. Install the tilt head.
2. Install the tilt head pivot pins.
3. Install the tilt spring. Refer to Tilt Spring - Assemble - Off Vehicle .
4. Align the race and upper shaft assembly (1) to the 12 o'clock position.
5. Put the lock cylinder in the lock position and remove the key.
6. Install the inner race (5).
7. Install the upper bearing inner race seat (4).
8. Install the upper bearing spring (3).
9. Lubricate the turn signal cancel cam assembly (2).
10. Install the turn signal cancel cam assembly (2).
11. Install the shaft lock shield assembly (1).
12. Install the bearing retaining using J 23653-SIR .
13. Remove J 23653-SIR from the steering column.
14. Install the SIR coil assembly. Refer to Inflatable Restraint Steering Wheel Module Coil Assemble - Off Vehicle .