For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Inspect the system for any loose components. Are any of the components loose? | -- | Go to Step 2 | Go to Step 3
2 | Tighten all of the loose fasteners to specifications. Is there a vibration or rattling noise? | -- | Go to Step 3 | System OK
3 | Inspect the system for any misaligned components. Are there any misaligned components? | -- | Go to Step 4 | --
4 | Align the system. Is there a vibration or rattling noise? | -- | Go to Step 5 | System OK
5 | Check for bent or damaged hangers, mounting brackets or clamps. Are any of these components bent or damaged? | -- | Go to Step 6 | System OK
6 | Repair or replace the bent or damaged hangers, mounting brackets or clamps. Is there a vibration or rattling noise? | -- | -- | System OK