For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
A/C Compressor Hose Block Fitting to Accumulator Bolt | 16 N·m | 11 lb ft
A/C Compressor Hose Block Fitting to Compressor Nut | 33 N·m | 24 lb ft
A/C Compressor Hose Block Fitting to Rear Suction Line Bolt | 16 N·m | 11 lb ft
Accumulator Strap Bolt | 5.5 N·m | 49 lb in
Air Distributor Case Cover | 1.6 N·m | 14 lb in
Air Inlet Housing Screws | 1.6 N·m | 14 lb in
Air Inlet Valve Electric Actuator Screws | 1.6 N·m | 14 lb in
Blower Motor Resistor/Relay Screws | 1.9 N·m | 16 lb in
Blower Motor Screws | 20 N·m | 15 lb ft
Center Air Distribution Duct Retaining Nuts | 10 N·m | 89 lb in
Compressor Mounting Bolts | 50 N·m | 37 lb ft
Compressor Shaft Nut | 18 N·m | 13 lb ft
Defroster Outlet Duct Retaining Screws | 10 N·m | 89 lb in
Heater A/C Module Bolts to Inside Passenger Compartment | 20 N·m | 15 lb ft
Heater A/C Module Nuts to Engine Compartment | 10 N·m | 89 lb in
Heater A/C Module Upper Mounting Screws | 1.6 N·m | 14 lb in
Heater Core Line Clip Screw | 1.6 N·m | 14 lb in
Heater Core Mounting Clip Screw | 1.6 N·m | 14 lb in
Heater Cover Screws | 1.6 N·m | 14 lb in
Heater Inlet Pipe Mounting Nut | 7 N·m | 62 lb in
Liquid Line at Block Fitting Bolt | 16 N·m | 12 lb ft
Rear A/C Line Block Fitting Bolt | 20 N·m | 15 lb ft
Rear Blower Motor Resistor Screws | 1.6 N·m | 14 lb in
Rear Heater A/C Module Mounting Bolts and Nut | 10 N·m | 89 lb in
Rear Heater Core Cover Screws | 3 N·m | 27 lb in
Rear Heater Core Line Bracket Bolt | 10 N·m | 89 lb in
Rear Temperature Valve Electric Actuator Screws | 1.6 N·m | 14 lb in
Refrigerant Line Bracket Nuts | 3.3 N·m | 29 lb in
Suction Line at Accumulator Fitting | 47 N·m | 35 lb ft
Suction Line at Block Fitting Bolt | 16 N·m | 12 lb ft
Thermostat Bypass Pipe Bolt to Cylinder Head | 25 N·m | 18 lb ft
Thermostat Bypass Pipe Bolt to Water Pump | 12 N·m | 106 lb in
Thermostat Bypass Pipe Nut | 25 N·m | 18 lb ft
Thermal Expansion Valve Bolts | 5 N·m | 44 lb in
Thermal Expansion Valve Line Bracket Bolt | 1.6 N·m | 14 lb in
Temperature Valve Electric Actuator Screws | 1.6 N·m | 14 lb in
Vacuum Tank Mounting Nuts | 10 N·m | 89 lb in