For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
Brake Fluid Level Indicator Switch | Right side of the brake fluid reservoir | Antilock Brake System Component Views in ABS/Traction Control | Instrument Panel, Gages, and Console Connector End Views in Instrument Panel and Console
Daytime Running Lamps (DRL) Control Module | Right of the steering column, behind the IP | Lighting Systems Component Views in Lighting Systems | Lighting Systems Connector End Views in Lighting Systems
Electronic Brake Control Module/Electronic Brake Traction Control Module (EBCM/EBTCM) | Left side of the IP, above the parking cable bracket | Antilock Brake System Component Views in ABS/Traction Control | Antilock Brake System Connector End Views in ABS/Traction Control
Fuse Block | Right side of the IP, in the right front door opening | Power and Grounding Component Views in Wiring System | --
Instrument Cluster | Left side of the IP | Instrument Panel, Gages, and Console Component Views in Instrument Panel and Console | Instrument Panel, Gages, and Console Connector End Views in Instrument Panel and Console
Park Brake Indicator Switch | Lower left A-pillar, part of the park brake assembly | Antilock Brake System Component Views in ABS/Traction Control | --
C203 (56 cavities) | IP wiring harness to the left side of the body wiring harness, left side of the steering column, below P101 | Harness Routing Views in SIR | Inline Harness Connector End Views in Wiring Systems
G200 | Right side of the IP, secured on the underside of the cross car beam, left of the heater-A/C vent | Harness Routing Views in SIR | --
P100 | On the right side of the bulkhead, left of the right strut tower | Harness Routing Views in SIR | --
S207 | IP harness, left side of IP approximately 4 cm (2 in) from the hazard lamp/turn signal flasher breakout | -- | --
S209 | IP harness, center of the IP approximately 8 cm (3 in) from the security indicator lamp breakout | -- | --
S230 | IP harness, right side of the IP approximately 4 cm (2 in) from the radio breakout | -- | --
S242 | IP harness, left side of the IP approximately 14 cm (6 in) from the radio and the rear window wiper/washer and multi-function switch breakout | -- | --