For 1990-2009 cars

#### Tools Required

J 35468 Oil Seal Installer

1. Install the front cover oil seal using the J 35468 .
2. Install the crankshaft position sensor.
3. Install the crankshaft position sensor screws.

Tighten
Tighten the crankshaft position sensor screws to 10 N·m (89 lb in).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

4. Install the water pump gasket.
5. Install the water pump.
6. Install the water pump bolts.

Tighten
Tighten the water pump bolts to 10 N·m (89 lb in).

7. Install the water pump pulley.
8. Install the water pump pulley bolts.

Tighten
Tighten the water pump pulley bolts to 25 N·m (18 lb ft).