For 1990-2009 cars

### Removal Procedure

Head restraints are the double-post type that are adjustable up or down. Only the solid-type head restraints have serviceable trim covers.

Removal of the head restraints can be accomplished by using the J 42372 or by fabricating a similar tool. The rear seat head restraint has only 1 locking post. Only one special tool or fabricated tool is necessary for the removal of the head restraint.

#### Tool Required

J 42372 Head Rest Removal Tool

1. Raise the head restraint to a full up position.
2. Push the head restraint down just far enough in order to center the locking clip (4) in the guide between the detents on the posts (3).
3. Insert the J 42372 down the detent side of the post (3).
4. Hold the tool down, and at the same time, lift the head restraint upward in order to disengage the detent (3) from the guide (4).
5. Lift the restraint out.

### Installation Procedure

1. Install the head restraint posts (1) into the guides.
2. Push the head restraint to a full down position.
3. Raise the head restraint in order to ensure that the restraint stops at the detent (3).
4. Return the head restraint to its original position.