For 1990-2009 cars

### Removal Procedure

1. Note the position of the fuel sender strainer (4) for installation.
2. Support the reservoir (2) with one hand and grasp the fuel sender strainer with the other hand.
3. Pull the fuel sender strainer (4) off of the fuel pump.
4. Inspect the fuel sender strainer. If the fuel sender strainer is contaminated, the fuel tank should be cleaned.
5. Discard the fuel sender strainer after inspection.
6. Remove the electrical connectors from the sensor assembly of the fuel pump and the cover assembly..
7. Remove the fuel level sensor (5) assembly.

### Installation Procedure

1. Install the fuel level sensor (5) assembly.
2. Install the electrical connectors to the fuel pump and the cover assembly.
3. Position the new fuel sender strainer (4) on the modular fuel sender (1) and push on the outer edge of the fuel sender strainer until the fuel sender strainer is fully seated.