For 1990-2009 cars

### Removal Procedure

Caution: Unless directed otherwise, the ignition and start switch must be in the OFF or LOCK position, and all electrical loads must be OFF before servicing any electrical component. Disconnect the negative battery cable to prevent an electrical spark should a tool or equipment come in contact with an exposed electrical terminal. Failure to follow these precautions may result in personal injury and/or damage to the vehicle or its components.

1. Disconnect the battery negative cable. Refer to Battery Negative Cable Disconnection and Connection in Engine Electrical.
2. Remove the left instrument panel insulator. Refer to Instrument Panel Insulator Panel Replacement - Left Side in Instrument Panel, Gauges and Console.
3. Disconnect the electrical connector from the switch (1).
4. Pull out the switch (1) in order to remove the switch (1) from the retainer in the brake pedal bracket.

### Installation Procedure

1. Push in the switch (1) in order to install the switch (1) to the retainer in the brake pedal bracket.
2. Connect the electrical connector to the switch (1).
3. Adjust the cruise control release switch and the stoplamp switch. Refer to Cruise Release Switch Adjustment .
4. Install the left instrument panel insulator. Refer to Instrument Panel Insulator Panel Replacement - Left Side in Instrument Panel, Gauges and Console.
5. Connect the battery negative cable. Refer to Battery Negative Cable Disconnection and Connection in Engine Electrical.