For 1990-2009 cars

#### Tools Required

• | J 33024 Clutch Coil Installer Adaptor

• | J 33025 Clutch Coil Puller Legs

• | J 8433 Compressor Pulley Puller

• | J 8433-3 Forcing Screw

1. Place the clutch coil assembly (1) on the front head with the clutch coil terminal at the positioned at the mark made during disassembly.
2. Place the J 33024 over the internal opening of the clutch coil housing and align installer with the compressor front head.
3. Install the J 8433-3 into the J 8433 and center the screw in the countersunk center hole of the J 33024 .
4. Install the 4 inch through bolts and washers from the J 42136 tool kit into the J 33025 and attach them to the compressor mounting bosses.
5. Turn the center forcing screw of the J 8433 to press the clutch coil onto the front head until the clutch coil is fully seated.

Make sure the clutch coil and the J 33024 stay in-line with each other while pressing the clutch coil onto the compressor.

6. Install the compressor clutch rotor and bearing assembly. Refer to Clutch Rotor and/or Bearing Install .
7. Install the compressor clutch plate and hub assembly. Refer to Compressor Clutch Plate/Hub Assembly Install .
8. Remove the compressor from the J 41790-A .