For 1990-2009 cars

### Removal Procedure

1. Turn the ignition OFF.
2. Remove the lower steering column shroud. Refer to Steering Column Shrouds - Disassemble .
3. Remove the shift lock control from the steering column. Refer to Automatic Transmission Shift Lock Control Disassemble - Off Vehicle .

### Installation Procedure

1. Install the shift lock control to the steering column. Refer to Automatic Transmission Shift Lock Control Assemble - Off Vehicle .
2. Remove the lower steering column shroud. Refer to Steering Column Shrouds - Assemble .