For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Antifreeze | GM Goodwrench DEX-COOL® or HAVOLINE® DEX-COOL®
Antifreeze to Water Ratio | 56% GM Goodwrench DEX-COOL® or HAVOLINE® DEX-COOL® to 44% Water
Coolant Freeze Point Protection | -35°C (-32°F) to -45°C (-48°F)
Cooling System Capacities

- Front HVAC System Only (C60) without Heavy Duty Cooling (V08)

9.1 liters

9.5 quarts

- Front and Rear HVAC System (C34) without Heavy Duty Cooling (V08)

11.6 liters

12.1 quarts

- Front HVAC System Only (C60) with Heavy Duty Cooling (V08)

10.1 liters

10.5 quarts

- Front and Rear HVAC System (C34) with Heavy Duty Cooling (V08)

12.6 liters

13.2 quarts

- Coolant Recovery Reservoir

0.99 liters

1 quart