For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
Body Control Module (BCM) | Below the right side of the IP, right of the IP compartment | Body Control System Component Views in Body Control System | Body Control System Connector End Views in Body Control System
Liftgate Lock (Ajar Indicator Switch) | Part of the liftgate lock assembly, inside the liftgate, below the license plate | Wiper/Washer Component Views in Wiper/Washer Systems | Power Door Systems Connector End Views in Doors
Powertrain Control Module (PCM) | Engine compartment, secured in the air cleaner assembly | Engine Controls Component Views in Engine Controls | Engine Controls Connector End Views in Engine Controls
Remote Control Door Lock Receiver (RCDLR) | Behind the center of the IP, underside of the IP trim, near the windsheild defrost vent | -- | --
Security Indicator Lamp | Center of the IP, mounted to the trim plate, near the windshield defrost vent | -- | Instrument Panel, Gages, and Console Connector End Views in Instrument Panel, Gauges and Console
Theft Deterrent Shock Sensor | Below the left side IP, right of the steering column | Theft Deterrent System Component Views | Theft Deterrent System Connector End Views
Underhood Accessory Wiring Junction Block | Engine compartment, front of the right wheelhouse, above the battery | Power and Grounding Component Views in Wiring Systems | Power and Grounding Connector End Views in Wiring Systems
C400 (2 cavities) | Body wiring harness to the liftgate wiring harness, above the right rear side of the roof headliner, near P406 and the liftgate | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C402 (8 cavities) | Body wiring harness to the liftgate wiring harness, above the right rear side of the roof headliner, near P406 and the liftgate | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
G200 | Right side of the IP, secured on the underside of the cross car beam, left of the heater-A/C vent | Harness Routing Views in Wiring Systems | --
G401 | Secured to the lower left D-pillar | Harness Routing Views in Wiring Systems | --
P100 | On the right side of the bulkhead, left of the right strut tower | Harness Routing Views in Wiring Systems | --
S202 | IP harness, leftt side of the IP approximately 18 cm (7 in) from the radio and rear window wiper/washer and multi-function switch breakout | -- | --
S211 | IP harness, left side of the IP approximately 18 cm (7 in) from the radio and the rear window wiper/washer and multi-function switch breakout | -- | --
S460 | Liftgate harness center of the liftgate approximately 7 cm (3 in) from the door lock cylinder switch breakout | -- | --