For 1990-2009 cars

## Front Bumper Fascia Replacement Chevy

### Removal Procedure

#### Tools Required

J 38778 Door Trim Pad and Garnish Clip Remover

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Remove both of the front tire and wheels. Refer to Tire Mounting and Dismounting in Tires and Wheels.
3. Remove the right and left front fender liner. Refer to Fender Liner Replacement in Body Front End.
4. Remove the front park/turn signal/side marker lamp. Refer to Hazard and Turn Signal Flasher Replacement in Lightning Systems And Horns.
5. Remove the push-in retainers from the upper and lower front bumper fascia.
6. Remove the front bumper fascia from the vehicle.

### Installation Procedure

1. Align the front bumper to the front impact bar and to the body.
2. Install the push-in retainers to the upper and lower front bumper fascia.
3. Install the front park/turn signal/sidemarker lamp. Refer to Hazard and Turn Signal Flasher Replacement in Lighting Systems and Horns.
4. Install the right and left front fender liner. Refer to Fender Liner Replacement in Body Front End.
5. Install both of the front tire and wheels. Refer to Tire Mounting and Dismounting in Tires and Wheels.
6. Lower the vehicle.

## Front Bumper Fascia Replacement Oldsmobile

### Removal Procedure

#### Tools Required

J 38778 Door Trim Pad and Garnish Clip Remover

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Remove both of the front tire and wheels. Refer to Tire Mounting and Dismounting in Tires and Wheels.
3. Remove the right and left front fender liner. Refer to Fender Liner Replacement in Body Front End.
4. Remove the front park/turn signal/side marker lamp. Refer to Hazard and Turn Signal Flasher Replacement in Lightning Systems And Horns.
5. Remove the push-in retainers from the upper and lower front bumper fascia.
6. Remove the front bumper fascia from the vehicle.

### Installation Procedure

1. Align the front bumper to the front impact bar and to the body.
2. Install the push-in retainers to the upper and lower front bumper fascia.
3. Install the front park/turn signal/sidemarker lamp. Refer to Hazard and Turn Signal Flasher Replacement in Lighting Systems and Horns.
4. Install the right and left front fender liner. Refer to Fender Liner Replacement in Body Front End.
5. Install both of the front tire and wheels. Refer to Tire Mounting and Dismounting in Tires and Wheels.
6. Lower the vehicle.

## Front Bumper Fascia Replacement Pontiac

### Removal Procedure

#### Tools Required

J 38778 Door Trim Pad and Garnish Clip Remover

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Remove both of the front tire and wheels. Refer to Tire Mounting and Dismounting in Tires and Wheels.
3. Remove the right and left front fender liner. Refer to Fender Liner Replacement in Body Front End.
4. Remove the front park/turn signal/side marker lamp. Refer to Hazard and Turn Signal Flasher Replacement in Lightning Systems And Horns.
5. Remove the push-in retainers from the upper and lower front bumper fascia.
6. Remove the front bumper fascia from the vehicle.

### Installation Procedure

1. Align the front bumper to the front impact bar and to the body.
2. Install the push-in retainers to the upper and lower front bumper fascia.
3. Install the front park/turn signal/sidemarker lamp. Refer to Hazard and Turn Signal Flasher Replacement in Lighting Systems and Horns.
4. Install the right and left front fender liner. Refer to Fender Liner Replacement in Body Front End.
5. Install both of the front tire and wheels. Refer to Tire Mounting and Dismounting in Tires and Wheels.
6. Lower the vehicle.