For 1990-2009 cars

### Removal Procedure

1. Remove the carpet. Refer to Floor Panel Carpet Replacement
2. Remove the floor pan insulators.

### Installation Procedure

Caution: All floor pan insulator material must meet Federal Vehicle Safety Standards for flammability. Failure to do so could result in personal injury and/or vehicle damage.

1. Install the floor pan insulators.
2. Install the carpet. Refer to Floor Panel Carpet Replacement .