For 1990-2009 cars

### Removal Procedure

1. Pull the outside rearview mirror from the mirror housing.

Do not damage the mirror.

2. Remove the outside rearview mirror. Refer to Power Mirror Replacement .
3. Remove the outside rearview mirror motor screws.
4. Remove the outside rearview mirror motor from the mirror housing.

### Installation Procedure

1. Install the outside rearview mirror motor to the mirror housing.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the outside rearview mirror motor screws.

Tighten
Tighten the screws to 10 N·m (89 lb in).

3. Install the outside rearview mirror. Refer to Power Mirror Replacement .
4. Push the outside rearview mirror to the mirror housing.

Do not damage the mirror.