For 1990-2009 cars

#### Tools Required

J 38778 Door Trim Pad Clip Remover

### Removal Procedure

1. Remove the upper seat belt anchor bolt from the belt guide loop.
2. Remove the body pillar upper trim panel retainers using the J 38778 .
3. Remove the upper trim panel from the body pillar by pulling the panel from the locator tabs.

### Installation Procedure

1. Align the locator tabs on the upper trim panel with the rear quarter trim panel.
2. Align the upper trim panel retainers with the holes and push to secure the panel to the vehicle.
3. Align the slider door seal to the body pillar upper trim panel if applicable.

Notice: Refer to Fastener Notice in the Preface section.

4. Install the upper seat belt anchor bolt to the belt guide loop.

Tighten
Tighten the bolt to 43 N·m (32 lb ft).