For 1990-2009 cars

The MAF sensor on this engine is attached to the throttle body assembly.

### Removal Procedure

1. Disconnet the MAF sensor electrical connector.
2. Remove the air inlet duct from MAF sensor.
3. Remove the MAF sensor from air filter housing.

### Installation Procedure

1. Carefully install MAF sensor to air inlet grommet.
2. Install the MAF sensor to air inlet duct.
3. Connect the electrical connector.