For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Initiate the self-calibration function or set the variance. Refer to Driver Information Center (DIC) or Message Center Operation . Does the compass display remain inoperative or inaccurate? | -- | Go to Step 2 | System OK
2 | Replace the driver information display module. Refer to Driver Information Center Replacement . Has the repair been made and the system rechecked? | -- | System OK | --