For 1990-2009 cars

### Removal Procedure

1. Remove the instrument panel. Refer to Instrument Panel Assembly Replacement in Instrument Panel, Gauges and Console.
2. Lift up on the retaining tab and rotate the air distribution extension duct.
3. Remove the air distribution extension duct from the instrument panel.

### Installation Procedure

1. Align the tabs of the air distribution extension duct with the slots in the instrument panel.
2. Rotate the air distribution extension duct to secure the retaining tab to the instrument panel.
3. Install the instrument panel. Refer to Instrument Panel Assembly Replacement in Instrument Panel, Gauges and Console