For 1990-2009 cars
ABS Components
Antilock Brake System Schematics
Handling ESD Sensitive Parts Notice

### Circuit Description

DTC 1261 identifies an ABS motor that cannot energize due to an open in the ABS motor circuitry. The malfunction will not allow proper front ABS operation.

### Conditions for Setting the DTC

DTC C1261 can only set when the motor is commanded off. A malfunction exists if the EBCM/EBTCM detects an out of range voltage on either of the right front ABS motor circuits. The out of range voltage on either circuit indicates an open circuit exists.

### Action Taken When the DTC Sets

• | An open ABS motor will not activate.

• | A malfunction DTC stores.

• | The ABS/TCS disables.

• | The amber ABS/TCS warning indicators turn on.

### Conditions for Clearing the DTC

• | The condition responsible for setting the DTC no longer exists and the Scan Tool Clear DTC function is used.

• | 100 drive cycles pass with no DTC detected.

### Diagnostic Aids

Use the Scan Tool Manual Control function in order to exercise ABS motor movement of affected channel in both directions while applying light pressure on the brake pedal. An intermittent malfunction may be indicated if erratic or jumpy brake pedal movement is detected while performing an apply or release function of the ABS monitor. Use the enhanced diagnostic function of the Scan Tool in order to measure the frequency of the malfunction. Refer to the Scan Tool manual or Scan Tool Diagnostics located in this section for the procedure.

If the malfunction is not current use the following procedure to pinpoint an intermittent malfunction in the motor circuitry or connections:

1. Wiggle the wires of the affected channel.
2. Inspect if the DTC resets.

Thoroughly inspect any circuitry that may be causing the intermittent complaint for the following conditions:

• | Rubbed-through wire insulation

• | A broken wire inside the insulation

• | Backed out terminals

• | Improper mating

• | Broken locks

• | Improperly formed or damaged terminals

• | Poor terminal-to-wiring connections

• | Physical damage to the wiring harness

Clear the DTCs after completing the diagnosis. Test drive the vehicle for three drive cycles in order to verify that the DTC does not reset. Use the following procedure in order to complete one drive cycle:

1. Start the vehicle.
2. Drive the vehicle over 16 km/h (10 mph).
3. Stop the vehicle.
4. Turn the ignition to the OFF position.

Important: Zero the J 39200 test leads before making any resistance measurements.

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Was the Diagnostic System Check performed? | -- | Go to Step 2 | Go to Diagnostic System Check
2 |

1. Install a scan tool.
2. Turn the ignition switch to the RUN position, engine off.

Does DTC C1261 occur intermittently?

--

Go to Diagnostic Aids

Go to Step 3

3 |

1. Turn the ignition switch to the OFF position.
2. Disconnect the 6-way ABS brake motor pack connector.
3. Use the J 39200 in order to measure the resistance between the 6-way ABS brake motor pack terminal A and 6-way ABS motor pack terminal B (leading to the RF brake motor).

Is the resistance within the specified range?

0.2-1.5ohms

Go to Step 4

Go to Step 8

4 |

1. Disconnect the 8-way EBCM/EBTCM connector C2.
2. Use J 39200 in order to measure the resistance between the 6-way ABS brake motor pack harness connector terminal B and the 8-way EBCM/EBTCM harness connector C2 terminal A.

Is the resistance within the specified range?

0-2ohms

Go to Step 5

Go to Step 9

5 | Use the J 39200 in order to measure the resistance between the 6-way ABS brake motor pack harness connector terminal A and the 8-way EBCM/EBTCM harness connector C2 terminal B. Is the resistance within the specified range? | 0-2ohms | Go to Step 6 | Go to Step 10
6 |

1. Inspect the following components for poor terminal contact and corrosion:

• | The 6-way ABS brake motor pack connector

• | The 6-way ABS brake motor pack harness connector

2. Inspect the following components for poor terminal contact and corrosion:

• | The 8-way EBCM/EBTCM connector C2

• | The 8-way EBCM/EBTCM harness connector C2

• | (Damage may cause a short to ground with the connector connected.)

Is there poor terminal contact or corrosion?

--

Go to Step 11

Go to Step 7

7 |

1. Reconnect the 6-way ABS brake motor pack connector.
2. Reconnect the 8-way EBCM/EBTCM connector C2.
3. Test drive the vehicle, obtaining a speed at least 16 km/h (10 mph).
4. Turn the ignition switch to the OFF position.
5. Repeat the drive sequence 2 additional times.
6. Use the Scan Tool in order to inspect for DTCs.

Did DTC C1261 set as a current DTC in the last three drive cycles?

--

Go to Step 12

Go to Step 13

8 | Replace the ABS brake motor pack. Refer to ABS Motor Pack Replacement . Is the repair complete? | -- | Go to Diagnostic System Check | --
9 | Repair the open in CKT 1282. Is the repair complete? | -- | Go to Diagnostic System Check | --
10 | Repair the open in CKT 1283. Is the repair complete? | -- | Go to Diagnostic System Check | --
11 | Replace all of the terminals and connectors that exhibit the following conditions:

• | Poor terminal contact

• | Corrosion

• | Damaged terminal(s)

Is the repair complete?

--

Go to Diagnostic System Check

--

12 | Replace the EBCM/EBTCM. Refer to Electronic Brake and Traction Control Module Replacement . Is the repair complete? | -- | Go to Diagnostic System Check | --
13 | The malfunction is intermittent or not present at this time. Is a concern still present? | -- | Go to Diagnostic Aids | Go to Diagnostic System Check