For 1990-2009 cars

# Warranty Admin. - March, 2000 Labor Time Guide Updates

Subject: | March, 2000 Labor Time Guide Updates

Models: | 1994-2000 Passenger Cars and Trucks

This bulletin addresses changes to the published General Motors Labor Time Guides. These changes (new or revised) are the result of new time studies and/or dealer "Requests For Review" being handled by the GM Service Operations Group. They are effective upon receipt. All changes will appear in the next printing of the Labor Time Guide.

Important: Please retain any changes made to the A, B, D and L Car Labor Time Guides as these vehicles have been discontinued since 1997 and the Labor Time Guides will not be republished. Changes to the P/H Truck Chassis should also be retained. The vehicle was discontinued in December, 1998. Please note: Labor Time Guides for these discontinued vehicles will not be republished.

#### LTG Update - C/K Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
94 | 95 | 96 | 97 | 98 | 99 | 00
YEAR VIN CODE
R | S | T | V | W | X | Y
BLADDER ASSEMBLY, PNEUMATIC SEAT - REPLACE

- PART GP: 11.378

- POLICY: S Additional .3 hours if the vehicle is delivered to and from the repair location

LUMBAR SEAT BACK |  |  |  |  |  |  |  |  |
PASSENGER |  | C7070 |  |  |  |  |  |  |
REMOVABLE SEAT BACK PANEL |  |  | -- | 0.3 | 0.3 | 0.3 | 0.3 | 0.3 | 0.3
NON-REMOVABLE SEAT BACK PANEL | R |  | -- | -- | -- | -- | 1.0 | 1.0 | 1.0
LUMBAR SEAT BACK |  |  |  |  |  |  |  |  |
DRIVER |  | C7071 |  |  |  |  |  |  |
REMOVABLE SEAT BACK PANEL |  |  | -- | 0.3 | 0.3 | 0.3 | 0.3 | 0.3 | 0.3
NON-REMOVABLE SEAT BACK PANEL | R |  | -- | -- | -- | -- | 1.0 | 1.0 | 1.0
SEAL, HUB OIL - REPLACE

- NOTE: See operation F1610, F1611, or F1617 for semi-floating axle shaft oil seal.

- NOTE: No Change to Labor Operation E4390 through E4397

ADD:

- A- W/Dual Wheels (Each Side)

0.1

0.1

0.1

0.1

0.1

0.1

0.1

B- To Replace Brake Shoes And Linings (Both Sides) |  |  |  |  |  |  |  |  |
W/Operations E4390 or E4391 (Full Floating only) | R |  | 1.1 | 1.1 | 1.1 | 1.1 | 1.1 | 1.1 | 1.1
W/Operation E4397 (Full Floating only) | R |  | 0.6 | 0.6 | 0.6 | 0.6 | 0.6 | 0.6 | 0.6
COVER AND/OR GASKET, TIMING - REPLACE

- PART GP: 0.206

- INC: Replace timing cover oil seal.

- NOTE: Applies to Engine Code J, N

R

J0780

2.6

2.6

2.7

2.7

2.7

2.7

2.7

No Change to "ADD" Condition |  |  |  |  |  |  |  |  |
*IND: N - New/R - Revised

#### LTG Update - K Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
94 | 95 | 96 | 97 | 98 | 99 | 00
YEAR VIN CODE
R | S | T | V | W | X | Y
REGULATOR, FRONT DOOR WINDOW - R&R OR REPLACE |  |  |  |  |  |  |  |  |
RIGHT POWER | N | C0182 | -- | -- | -- | -- | 0.8 | 0.8 | 0.8
LEFT POWER | N | C0183 | -- | -- | -- | -- | 0.8 | 0.8 | 0.8
ADD:

- A- Diagnosis Time: You may claim 0.0 to 0.3 hours depending on actual time performing diagnosis

N

--

--

--

--

0-.3

0-.3

0-.3

REGULATOR, REAR DOOR WINDOW - R&R OR REPLACE |  |  |  |  |  |  |  |  |
RIGHT POWER | N | C0382 | -- | -- | -- | -- | 0.7 | 0.7 | 0.7
LEFT POWER | N | C0383 | -- | -- | -- | -- | 0.7 | 0.7 | 0.7
ADD:

- A- Diagnosis Time: You may claim 0.0 to 0.3 hours depending on actual time performing diagnosis

N

--

--

--

--

0-.3

0-.3

0-.3

*IND: N - New/R - Revised

#### LTG Update - Ksp Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
94 | 95 | 96 | 97 | 98 | 99 | 00
YEAR VIN CODE
R | S | T | V | W | X | Y
SENSOR, CRANKSHAFT POSITION - REPLACE |  | J4355 | 0.4 | 0.4 | 0.4 | 0.4 | 0.3 | 0.3 | 0.3
ADD:

- A- To Replace Both

N

--

0.1

0.1

0.1

0.1

0.1

0.1

B- Diagnosis Time: You may claim 0.0 to 0.3 hours depending on actual time performing diagnosis |  |  | 0-.3 | 0-.3 | 0-.3 | 0-.3 | 0-.3 | 0-.3 | 0-.3
*IND: N - New/R - Revised

#### LTG Update - S/T Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
94 | 95 | 96 | 97 | 98 | 99 | 00
YEAR VIN CODE
R | S | T | V | W | X | Y
VALVE BODY - R&R OR REPLACE

- PART GP: 4.265

- NOTE: Applies to 4L60E

R

K6560

1.2

1.1

1.1

1.1

1.1

1.1

1.1

No Change to "ADD" Conditions |  |  |  |  |  |  |  |  |
SWITCHES, STEERING WHEEL - REPLACE |  |  |  |  |  |  |  |  |
AUDIO SYSTEM CONTROL | N | R0742 | -- | -- | 0.5 | 0.5 | 0.5 | 0.5 | 0.5
ADD:

- A- Diagnosis Time: You may claim 0.0 to 0.3 hours depending on actual time performing diagnosis

--

--

0-.3

0-.3

0-.3

0-.3

0-.3

*IND: N - New/R - Revised

#### LTG Update - U/X Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
94 | 95 | 96 | 97 | 98 | 99 | 00
YEAR VIN CODE
R | S | T | V | W | X | Y
BELT, SAFETY FRONT (BUCKLE SIDE) - REPLACE

- PART GP: 14.875

RIGHT |  | C9020 | 0.6 | 0.6 | 0.6 | 0.6 | 0.7 | 0.7 | 0.7
LEFT |  | C9021 | 0.6 | 0.6 | 0.6 | 0.6 | 0.6 | 0.6 | 0.6
ADD:

- A- Diagnosis Time: You may claim 0.0 to 0.3 hours depending on actual time performing diagnosis

N

0-.3

0-.3

0-.3

0-.3

0-.3

0-.3

0-.3

NOTE: Applies to C9021 only | N |  |  |  |  |  |  |  |
PUMP, SECONDARY AIR INJECTION - REPLACE

- PART GP: 3.660

- POLICY: E (7/70 California - Includes other applicable states)

N

J6050

--

--

--

--

--

--

0.6

ADD:

- A- Diagnosis Time: You may claim 0.0 to 0.3 hours depending on actual time performing diagnosis

--

--

--

--

--

--

0-.3

*IND: N - New/R - Revised

#### LTG Update - V Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
94 | 95 | 96 | 97 | 98 | 99 | 00
YEAR VIN CODE
R | S | T | V | W | X | Y
BALANCER, HARMONIC - REPLACE

- NOTE: Applies to Engine Code R

R

J0720

--

--

--

0.5

0.5

0.5

0.5

*IND: N - New/R - Revised

#### LTG Update - W Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
94 | 95 | 96 | 97 | 98 | 99 | 00
YEAR VIN CODE
R | S | T | V | W | X | Y
BELT, SAFETY FRONT (RETRACTOR SIDE) - R&R OR REPLACE

- PART GP: 14.875

- NOTE: No Change to Labor Operation C9040 or C9041

BOTH |  | C9047 |  |  |  |  |  |  |
2 DOOR |  |  |  |  |  |  |  |  |
EXC MONTE CARLO |  |  | 1.2 | 1.2 | 1.2 | 1.2 | 1.2 | 1.2 | 1.2
MONTE CARLO |  |  | -- | 1.2 | 1.2 | 1.2 | 1.2 | 1.2 | 0.6
4 DOOR |  |  |  |  |  |  |  |  |
CHEVROLET |  |  |  |  |  |  |  |  |
LUMINA |  |  | 1.2 | 1.2 | 1.2 | 1.2 | 1.2 | 1.2 | 1.2
IMPALA |  |  | -- | -- | -- | -- | -- | -- | 0.9
PONTIAC/BUICK/OLDSMOBILE | R |  | 1.2 | 1.2 | 1.2 | 1.0 | 1.0 | 1.0 | 1.0
ACTUATOR AND/OR MOTOR, ELECTRIC - REPLACE

- PART GP: 9.779

- NOTE: Applies only to electronic A/C equipped vehicles

TEMPERATURE DOOR |  |  |  |  |  |  |  |  |
RIGHT | R | D1811 |  |  |  |  |  |  |
EXC CHEVROLET |  |  | 0.6 | 0.6 | 0.6 | 0.4 | 0.4 | 0.4 | 0.4
CHEVROLET |  |  |  |  |  |  |  |  |
LUMINA |  |  | 0.6 | 0.6 | 0.6 | 0.4 | 0.4 | 0.4 | 0.4
MONTE CARLO |  |  | -- | 0.6 | 0.6 | 0.4 | 0.4 | 0.4 | 0.3
IMPALA |  |  | -- | -- | -- | -- | -- | -- | 0.3
TEMPERATURE DOOR |  |  |  |  |  |  |  |  |
LEFT | R | D1812 |  |  |  |  |  |  |
EXC CHEVROLET |  |  | -- | -- | -- | 0.6 | 0.6 | 0.6 | 0.6
CHEVROLET |  |  | -- | -- | -- | 0.6 | 0.6 | 0.6 | 0.4
ADD:

- A- Diagnosis Time: You may claim 0.0 to 0.3 hours depending on actual time performing diagnosis

0-.3

0-.3

0-.3

0-.3

0-.3

0-.3

0-.3

COMPRESSOR ASSEMBLY - REPLACE

- PART GP: 9.170

D4440

ENGINE CODE H | R |  | -- | -- | -- | -- | -- | 2.1 | 2.1
ENGINE CODE K AND 1 |  |  | 0.8 | 0.8 | 0.8 | 0.7 | 0.7 | 0.7 | 0.7
ENGINE CODE X |  |  | 1.1 | 1.1 | 1.1 | 1.1 |  |  |
ENGINE CODE M, T, J AND E |  |  | 0.8 | 0.8 | 0.8 | 0.8 | 0.8 | 0.8 | 0.8
No Change to "ADD" Conditions |  |  |  |  |  |  |  |  |
SWITCH - REPLACE

- No Change to "NOTEs," "PART GPs," or "INCs"

- No Change to Labor Operations N2050 through N2280

HEADLAMP |  | N2290 |  |  |  |  |  |  |
CHEVROLET | R |  | 0.2 | 0.2 | 0.4 | 0.4 | 0.4 | 0.4 | 0.4
PONTIAC |  |  | 0.2 | 0.2 | 0.2 | 0.8 | 0.8 | 0.8 | 0.8
OLDSMOBILE |  |  | 0.2 | 0.2 | 0.2 | 0.2 | 0.8 | 0.8 | 0.8
BUICK |  |  | 0.2 | 0.2 | 0.2 | 0.8 | 0.8 | 0.8 | 0.8
NOTE: No Change to Labor Operations N2310 through N2625 |  |  |  |  |  |  |  |  |
*IND: N - New/R - Revised