For 1990-2009 cars

# CAMPAIGN:SHIFT CABLE RETAINING TABS BREAKING

#### NOTE: GM OF CANADA VERSION OF 98023 IS LOCATED BELOW THE US VERSION ______________________________________________________________________ PRODUCT CAMPAIGNS 98023 JUNE, 1998

PRODUCT RECALL CAMPAIGN

FMVSS NON-COMPLIANCE CAMPAIGN

#### SUBJECT: 98023 - SHIFT CABLE RETAINING TABS BREAKING AND SWIVEL TUBE BECOMES DETACHED FROM END FITTING

#### MODELS: 1998 CHEVROLET VENTURE, OLDSMOBILE SILHOUETTE, PONTIAC TRANS SPORT EQUIPPED WITH 3.4L-V6 ENGINE AND AUTOMATIC TRANSMISSION

THE HIGHWAY SAFETY ACT, AS AMENDED, PROVIDES THAT EACH VEHICLE WHICH IS SUBJECT TO A RECALL CAMPAIGN OF THIS TYPE MUST BE ADEQUATELY REPAIRED WITHIN A REASONABLE TIME AFTER THE CUSTOMER HAS TENDERED IT FOR REPAIR. A FAILURE TO REPAIR WITHIN SIXTY (60) DAYS AFTER TENDER OF A VEHICLE IS PRIMA FACIE EVIDENCE OF FAILURE TO REPAIR WITHIN A REASONABLE TIME.

IF THE CONDITION IS NOT ADEQUATELY REPAIRED WITHIN A REASONABLE TIME, THE CUSTOMER MAY BE ENTITLED TO AN IDENTICAL OR REASONABLY EQUIVALENT VEHICLE AT NO CHARGE OR TO A REFUND OF THE PURCHASE PRICE LESS A REASONABLE ALLOWANCE FOR DEPRECIATION.

TO AVOID HAVING TO PROVIDE THESE BURDENSOME REMEDIES, EVERY EFFORT MUST BE MADE TO PROMPTLY SCHEDULE AN APPOINTMENT WITH EACH CUSTOMER AND TO REPAIR THEIR VEHICLE AS SOON AS POSSIBLE. AS YOU WILL SEE IN READING THE ATTACHED COPY OF THE DIVISIONAL LETTER THAT IS BEING SENT TO CUSTOMERS, THE CUSTOMERS ARE BEING INSTRUCTED TO CONTACT THE APPROPRIATE CUSTOMER ASSISTANCE CENTER IF THEIR DEALER DOES NOT REMEDY THE CONDITION WITHIN FIVE (5) DAYS OF THE MUTUALLY AGREED UPON SERVICE DATE. IF THE CONDITION IS NOT REMEDIED WITHIN A REASONABLE TIME, THEY ARE INSTRUCTED ON HOW TO CONTACT THE NATIONAL HIGHWAY TRAFFIC SAFETY ADMINISTRATION.

DEFECT INVOLVED

GENERAL MOTORS HAS DECIDED THAT CERTAIN 1998 U-VANS EQUIPPED WITH 3.4L-V6 (LA1) ENGINES AND AUTOMATIC (M13) TRANSMISSIONS FAIL TO CONFORM TO THE FEDERAL MOTOR VEHICLE SAFETY STANDARD 102. THESE VEHICLES MAY HAVE (1) A BROKEN SHIFT CABLE FITTING OR (2) LOOSE SHIFT LINKAGE SWIVEL TUBES. WITH EITHER CONDITION, MOVING THE SHIFT LEVER TO PARK MAY NOT SHIFT THE TRANSMISSION TO PARK. THE VEHICLE COULD ROLL AND A CRASH COULD OCCUR WITHOUT PRIOR WARNING. TO HELP AVOID THIS, WHEN YOU SHIFT TO PARK, ALWAYS APPLY THE PARK BRAKE BEFORE YOU RELEASE THE SERVICE BRAKE.

VEHICLES INVOLVED

INVOLVED ARE ALL 1998 U-VANS MODEL VEHICLES EQUIPPED WITH OPTION CODES LA1 (3.4L V-6 ENGINES) AND M13 (AUTOMATIC TRANSMISSION) AND BUILT WITHIN THE FOLLOWING VIN BREAKPOINTS:

YEAR DIVISION MODEL PLANT CODE FROM THROUGH 1998 ALL U-VAN DORAVILLE "D" WD152963 WD241250

#### NOTICE: DEALERS SHOULD CONFIRM VEHICLE ELIGIBILITY THROUGH VISS (VEHICLE INFORMATION SERVICE SYSTEM) PRIOR TO BEGINNING CAMPAIGN REPAIRS. NOT ALL VEHICLES WITHIN THE ABOVE BREAKPOINTS MAY BE INVOLVED.

INVOLVED VEHICLES HAVE BEEN IDENTIFIED BY VEHICLE IDENTIFICATION NUMBER. COMPUTER LISTINGS CONTAINING THE COMPLETE VEHICLE IDENTIFICATION NUMBER, CUSTOMER NAME AND ADDRESS DATA HAVE BEEN PREPARED, AND ARE BEING FURNISHED TO INVOLVED DEALERS WITH THE CAMPAIGN BULLETIN. THE CUSTOMER NAME AND ADDRESS DATA FURNISHED WILL ENABLE DEALERS TO FOLLOW-UP WITH CUSTOMERS INVOLVED IN THIS CAMPAIGN. ANY DEALER NOT RECEIVING A COMPUTER LISTING WITH THE CAMPAIGN BULLETIN HAS NO INVOLVED VEHICLES CURRENTLY ASSIGNED.

THESE DEALER LISTINGS MAY CONTAIN CUSTOMER NAMES AND ADDRESSES OBTAINED FROM STATE MOTOR VEHICLE REGISTRATION RECORDS. THE USE OF SUCH MOTOR VEHICLE REGISTRATION DATA FOR ANY OTHER PURPOSE IS A VIOLATION OF LAW IN SEVERAL STATES. ACCORDINGLY, YOU ARE URGED TO LIMIT THE USE OF THIS LISTING TO THE FOLLOW-UP NECESSARY TO COMPLETE THIS CAMPAIGN.

PARTS INFORMATION

PARTS REQUIRED TO COMPLETE THIS CAMPAIGN ARE TO BE OBTAINED FROM GENERAL MOTORS SERVICE PARTS OPERATIONS (GMSPO). PLEASE REFER TO YOUR "INVOLVED VEHICLES LISTING" PRIOR TO ORDERING REQUIREMENTS. NORMAL ORDERS SHOULD BE PLACED ON A DRO = DAILY REPLENISHMENT ORDER. AN EMERGENCY REQUIREMENT SHOULD BE ORDERED ON A CSO = CUSTOMER SPECIAL ORDER.

PART NUMBER DESCRIPTION QUANTITY/ VEHICLE

12562038 CABLE ASSY, AUTO TRANS SHIFT 1

#### NOTICE: IT IS ESTIMATED THAT ONLY 10% OF INVOLVED VEHICLES WILL REQUIRE CABLE ASSEMBLY REPLACEMENT. PLEASE ORDER PARTS ACCORDINGLY.

CUSTOMER NOTIFICATION

CUSTOMERS WILL BE NOTIFIED OF THIS CAMPAIGN ON THEIR VEHICLES BY GENERAL MOTORS (SEE COPY OF TYPICAL CUSTOMER LETTER INCLUDED WITH THIS BULLETIN - ACTUAL DIVISIONAL LETTER MAY VARY SLIGHTLY).

DEALER CAMPAIGN RESPONSIBILITY

ALL UNSOLD NEW VEHICLES IN DEALERS' POSSESSION AND SUBJECT TO THIS CAMPAIGN MUST BE HELD AND INSPECTED/REPAIRED PER THE SERVICE PROCEDURE OF THIS CAMPAIGN BULLETIN BEFORE CUSTOMERS TAKE POSSESSION OF THESE VEHICLES.

DEALERS ARE TO SERVICE ALL VEHICLES SUBJECT TO THIS CAMPAIGN AT NO CHARGE TO CUSTOMERS, REGARDLESS OF MILEAGE, AGE OF VEHICLE, OR OWNERSHIP, FROM THIS TIME FORWARD.

CUSTOMERS WHO HAVE RECENTLY PURCHASED VEHICLES SOLD FROM YOUR VEHICLE INVENTORY, AND FOR WHICH THERE IS NO CUSTOMER INFORMATION INDICATED ON THE DEALER LISTING, ARE TO BE CONTACTED BY THE DEALER. ARRANGEMENTS ARE TO BE MADE TO MAKE THE REQUIRED CORRECTION ACCORDING TO THE INSTRUCTIONS CONTAINED IN THIS BULLETIN. THIS COULD BE DONE BY MAILING TO SUCH CUSTOMERS A COPY OF THE APPROPRIATE DIVISIONAL CUSTOMER LETTER ACCOMPANYING THIS BULLETIN. CAMPAIGN FOLLOW-UP CARDS SHOULD NOT BE USED FOR THIS PURPOSE, SINCE THE CUSTOMER MAY NOT AS YET HAVE RECEIVED THE NOTIFICATION LETTER.

IN SUMMARY, WHENEVER A VEHICLE SUBJECT TO THIS CAMPAIGN ENTERS YOUR VEHICLE INVENTORY, OR IS IN YOUR DEALERSHIP FOR SERVICE IN THE FUTURE, PLEASE TAKE THE STEPS NECESSARY TO BE SURE THE CAMPAIGN CORRECTION HAS BEEN MADE BEFORE SELLING OR RELEASING THE VEHICLE.

THIS BULLETIN IS NOTICE TO YOU THAT THE NEW MOTOR VEHICLES INCLUDED IN THIS CAMPAIGN MAY NOT COMPLY WITH THE STANDARD IDENTIFIED ABOVE. UNDER 41 U.S.C. SECTION 30112 OF THE HIGHWAY SAFETY ACT AS AMENDED, IT IS ILLEGAL FOR A DEALER TO SELL A NEW MOTOR VEHICLE WHICH THE DEALER KNOWS DOES NOT COMPLY WITH AN APPLICABLE FEDERAL MOTOR VEHICLE SAFETY STANDARD. AS A CONSEQUENCE, IF YOU SELL ANY OF THESE MOTOR VEHICLES WITHOUT FIRST PERFORMING THE CAMPAIGN CORRECTION, YOUR DEALERSHIP MAY BE SUBJECT TO A CIVIL PENALTY UP TO $1,000 FOR EACH SUCH SALE.

SERVICE PROCEDURE

THE CAMPAIGN SERVICE PROCEDURE INVOLVES INSPECTION OF THE AUTOMATIC TRANSAXLE RANGE SELECTOR CABLE, THEN IF NECESSARY, REPLACEMENT OF THE SHIFT CABLE.

INSPECTION PROCEDURE. ALL VEHICLES.

1. SET THE PARKING BRAKE.

2. BLOCK THE WHEELS

3. REMOVE PUSH-IN RETAINERS FROM DRIVER SIDE INSTRUMENT PANEL INSULATOR TO INSTRUMENT PANEL.

4. REMOVE PRESS-ON RETAINERS FROM DRIVER SIDE INSTRUMENT PANEL INSULATOR TO DASH MAT.

5. REMOVE INSTRUMENT PANEL COURTESY LAMP BY UNSNAPPING FROM INSTRUMENT PANEL INSULATOR.

6. REMOVE INSTRUMENT PANEL INSULATOR FROM INSTRUMENT PANEL.

7. REMOVE BOLTS/SCREWS FROM BOTTOM OF KNEE BOLSTER.

8. REMOVE KNEE BOLSTER BY PULLING TO RELEASE UPPER CLIPS.

9. SHIFT THE STEERING COLUMN TRANSMISSION SHIFT LEVER INTO THE LOW GEAR (L1) POSITION.

#### NOTE: THE VEHICLE DOES NOT HAVE TO BE STARTED OR RUNNING, BUT THE IGNITION KEY MUST BE IN THE "ACCESSORY" OR IN THE "ON" POSITION IN ORDER TO MOVE THE STEERING COLUMN TRANSMISSION SHIFT LEVER.

10. INSPECT SWIVEL TUBE RETENTION BY PULLING THE BLACK PLASTIC TUBE UPWARDS TOWARDS THE STEERING WHEEL.

#### NOTE: EXCESSIVE FORCE IS NOT REQUIRED TO VERIFY PROPER RETENTION OF THE TUBE TO THE CABLE CONDUIT FITTING. IF THE SWIVEL TUBE IS NOT PROPERLY SEATED IT CAN BE DISLODGED WITH A RELATIVELY LIGHT AXIAL FORCE (LESS THAN 80 N (20 LBS)). THIS CAN BE ACCOMPLISH-ED BY USING TWO OR THREE FINGERS TO PULL UPWARDS ON THE TUBE TO VERIFY RETENTION.

11. VISUALLY INSPECT FOR BROKEN, CRACKED, OR MISSING RETAINING TABS ON THE SHIFT CABLE CONDUIT FITTING AT THE STEERING COLUMN BRACKET.

12. INSPECT FOR PRESENCE OF THE CABLE RETAINER THAT HOLDS THE PLASTIC TABS OF THE CABLE FITTING AGAINST THE BRACKET. THE CABLE RETAINER IS SHAPED LIKE A LARGE STAPLE.

13. IF UPON INSPECTION, THE SWIVEL TUBE CAN BE DISLODGED OR BECOMES DISCONNECTED, OR THE RETAINING TABS ARE CRACKED OR MISSING, OR THE CABLE RETAINER IS MISSING, THE SHIFT CABLE MUST BE REPLACED. FOLLOW THE AUTOMATIC TRANSAXLE RANGE SELECTOR CABLE REMOVAL, INSTALLATION, AND ADJUSTMENT PROCEDURE STARTING WITH STEP 25. OTHERWISE, CONTINUE WITH STEP 14 TO RE-INSTALL THE KNEE BOLSTER AND THE INSTRUMENT PANEL INSULATOR.

#### NOTICE: REFER TO FASTENER NOTICE IN CAUTIONS AND NOTICES.

14. SHIFT THE STEERING COLUMN TRANSMISSION SHIFT LEVER INTO THE "PARK" POSITION.

15. TURN IGNITION KEY TO THE OFF POSITION.

16. INSTALL KNEE BOLSTER TO INSTRUMENT PANEL BY LOCATING CLIPS TO SLOTS INSTRUMENT PANEL AND PUSHING TO SECURE.

17. INSTALL BOLTS/SCREWS TO BOTTOM OF KNEE BOLSTER. TIGHTEN BOLTS/SCREWS TO 2.5 NM. (22 LB. IN.)

18. INSTALL INSTRUMENT PANEL COURTESY LAMP BY SNAPPING INTO INSTRUMENT PANEL INSULATOR.

19. POSITION INSTRUMENT PANEL INSULATOR TO INSTRUMENT PANEL.

20. INSTALL PRESS-ON RETAINERS TO INSTRUMENT PANEL INSULATOR TO DASH MAT.

21. INSTALL PUSH-IN RETAINERS TO INSTRUMENT PANEL INSULATOR TO INSTRUMENT PANEL.

22. UNBLOCK WHEELS.

23. RELEASE THE PARKING BRAKE WHILE APPLYING THE SERVICE BRAKE.

24. INSTALL THE GM CAMPAIGN IDENTIFICATION LABEL.

AUTOMATIC TRANSAXLE RANGE SELECTOR CABLE REMOVAL, INSTALLATION, AND ADJUSTMENT REMOVAL

25. REMOVE THE THROTTLE BODY AIR INLET DUCT.

26. REMOVE THE AUTOMATIC TRANSAXLE RANGE SELECTOR CABLE FROM THE AUTOMATIC TRANSAXLE RANGE SELECTOR MANUAL LEVER.

27. REMOVE RETAINER FROM THE AUTOMATIC TRANSAXLE RANGE SELECTOR CABLE.

28. REMOVE THE AUTOMATIC TRANSAXLE RANGE SELECTOR CABLE FROM THE AUTOMATIC TRANSAXLE RANGE SELECTOR CABLE BRACKET.

29. REMOVE THE DRIVER SIDE INSTRUMENT PANEL INSULATOR. (IF NOT ALREADY REMOVED DURING INSPECTION PROCEDURE.) SEE PROCEDURE STEPS 3 - 8 ABOVE.

30. REMOVE THE KNEE BOLSTER. (IF NOT ALREADY REMOVED DURING INSPECTION PROCEDURE.) SEE PROCEDURE STEPS 3 - 8 ABOVE.

31. REMOVE THE AUTOMATIC TRANSAXLE RANGE SELECTOR CABLE FROM THE COLUMN CONTROL LEVER BALL STUD.

32. REMOVE CABLE RETAINER FROM AUTOMATIC TRANSAXLE RANGE SELECTOR CABLE.

33. REMOVE THE AUTOMATIC TRANSAXLE RANGE SELECTOR CABLE FROM THE STEERING COLUMN BRACKET.

34. REMOVE THE AUTOMATIC TRANSAXLE RANGE SELECTOR CABLE THROUGH THE HOLE IN THE COWL.

INSTALLATION

35. PROPERLY ROUTE THE NEW AUTOMATIC TRANSAXLE RANGE SELECTOR CABLE THROUGH THE ENGINE COMPARTMENT.

36. PROPERLY ROUTE THE AUTOMATIC TRANSAXLE RANGE SELECTOR CABLE THROUGH THE COWL.

37. INSTALL THE AUTOMATIC TRANSAXLE RANGE SELECTOR CABLE TO THE STEERING COLUMN BRACKET.

38. INSTALL CABLE RETAINER TO THE CABLE FITTING AGAINST THE STEERING COLUMN BRACKET.

39. INSTALL THE AUTOMATIC TRANSAXLE RANGE SELECTOR CABLE TO THE COLUMN CONTROL LEVER BALL STUD.

40. INSTALL THE AUTOMATIC TRANSAXLE RANGE SELECTOR CABLE TO THE AUTOMATIC TRANSAXLE RANGE SELECTOR CABLE BRACKET.

41. INSTALL THE CABLE RETAINER TO THE CABLE ADJUSTER FITTING AGAINST THE AUTOMATIC TRANSAXLE RANGE SELECTOR CABLE BRACKET.

42. INSTALL THE AUTOMATIC TRANSAXLE RANGE SELECTOR CABLE TO THE AUTOMATIC TRANSAXLE RANGE SELECTOR LEVER BALL STUD.

CABLE ADJUSTMENT

#### NOTICE: ADJUST THE AUTOMATIC TRANSAXLE RANGE SELECTOR CABLE WHILE THE TRANSAXLE AND THE GEAR SELECTOR ARE IN THE NEUTRAL POSITION ONLY. FAILURE TO DO SO MAY CAUSE MIS-ADJUSTMENT.

43. USE APPROPRIATE TOOL TO PRY ON THE AUTOMATIC TRANSAXLE RANGE SELECTOR CABLE TERMINAL AT THE AUTOMATIC TRANSAXLE RANGE SELECTOR LEVER TO REMOVE THE AUTOMATIC TRANSAXLE RANGE SELECTOR CABLE TERMINAL FROM THE TRANSAXLE MANUAL SHAFT LEVER PIN.

#### NOTICE: DO NOT PRY AND DO NOT PULL UP ON ANY OTHER PART OF THE AUTOMATIC TRANSAXLE RANGE SELECTOR CABLE OR DAMAGE MAY OCCUR.

44. FULLY LIFT UP THE ADJUSTER LOCK BUTTON. ENSURE THE ADJUSTER IS FREE TO MOVE.

ADJUSTER IS NEXT TO THE CABLE RETAINER LOCATED AT THE TRANSAXLE SIDE OF THE AUTOMATIC TRANSAXLE RANGE SELECTOR CABLE.

45. ROTATE THE AUTOMATIC TRANSAXLE RANGE SELECTOR MANUAL LEVER (LOCATED AT THE TRANSAXLE) FULLY COUNTERCLOCKWISE TO THE "PARK" GEAR POSITION, THEN ROTATE THE LEVER CLOCKWISE TWO (2) CLICKS INTO THE "NEUTRAL" GEAR TO PLACE THE AUTOMATIC TRANSAXLE RANGE SELECTOR MANUAL LEVER IN THE "NEUTRAL" GEAR POSITION.

46. PERFORM THE FOLLOWING STEPS TO PLACE THE STEERING COLUMN SHIFTER LEVER INTO THE "NEUTRAL" POSITION:

46.1 ROTATE THE SHIFT LEVER TO THE "LOW 1" (L1) POSITION, FULLY DOWN.

46.2 PUSH FORWARD ON THE LEVER WHILE SLOWLY PUSHING UP. THE GEAR SHIFT LEVER WILL MOVE UP WHILE CLICKING OVER THE GEAR OVER TRAVEL STOPS.

46.3 RELEASE THE GEAR SHIFT ONCE THE GEAR SHIFT LEVER STOPS SOLIDLY. THE GEAR SHIFT LEVER IS NOW IN THE "NEUTRAL" POSITION.

47. GRASP THE AUTOMATIC TRANSAXLE RANGE SELECTOR CABLE TERMINAL IN THE UNDERHOOD AREA.

48. PULL THE AUTOMATIC TRANSAXLE RANGE SELECTOR CABLE TERMINAL TOWARDS THE BALL STUD ON THE AUTOMATIC TRANSAXLE RANGE SELECTOR MANUAL LEVER. THE TRANSAXLE RANGE SELECTOR CABLE ADJUSTER SPRING SHOULD COMPRESS AS THE TERMINAL IS MOVED TOWARD THE PIN.

49. CAREFULLY PUSH DOWN ON THE TERMINAL UNTIL THE TERMINAL SNAPS TO ATTACH THE TERMINAL TO THE AUTOMATIC TRANSAXLE RANGE SELECTOR MANUAL LEVER BALL STUD.

DO NOT MOVE THE AUTOMATIC TRANSAXLE RANGE SELECTOR MANUAL LEVER OUT OF POSITION WHILE PERFORMING THIS PROCEDURE.

DO NOT PULL THE TERMINAL BEYOND THE PIN THEN PUSH BACK OR THE STEERING COLUMN SHIFTER MAY MOVE OUT OF THE "NEUTRAL" POSITION.

50. PRESS THE ADJUSTER LOCK BUTTON DOWN FLUSH WITH THE ADJUSTER BODY.

51. SHIFT TO "PARK".

52. UNBLOCK WHEELS.

53. RELEASE THE PARKING BRAKE WHILE APPLYING THE SERVICE BRAKE.

54. START THE ENGINE.

55. ENSURE ALL THE INDICATED GEAR POSITIONS MATCH THE VEHICLE RESPONSE.

56. SHIFT TRANSAXLE TO "PARK".

57. TURN THE IGNITION KEY TO THE OFF POSITION.

58. INSTALL THE THROTTLE BODY AIR INLET DUCT.

#### NOTICE: REFER TO FASTENER NOTICE IN CAUTIONS AND NOTICES.

59. INSTALL KNEE BOLSTER TO INSTRUMENT PANEL BY LOCATING CLIPS TO SLOTS INSTRUMENT PANEL AND PUSHING TO SECURE.

60. INSTALL BOLTS/SCREWS TO BOTTOM OF KNEE BOLSTER. TIGHTEN BOLTS/SCREWS TO 2.5 NM. (22 LB. IN.)

61. INSTALL INSTRUMENT PANEL COURTESY LAMP BY SNAPPING INTO INSTRUMENT PANEL INSULATOR.

62. POSITION INSTRUMENT PANEL INSULATOR TO INSTRUMENT PANEL.

63. INSTALL PRESS-ON RETAINERS TO INSTRUMENT PANEL INSULATOR TO DASH MAT.

64. INSTALL PUSH-IN RETAINERS TO INSTRUMENT PANEL INSULATOR TO INSTRUMENT PANEL.

65. INSTALL THE GM CAMPAIGN IDENTIFICATION LABEL

CAMPAIGN IDENTIFICATION LABEL

EACH VEHICLE CORRECTED IN ACCORDANCE WITH THE INSTRUCTIONS OUTLINED IN THIS PRODUCT CAMPAIGN BULLETIN WILL REQUIRE A "CAMPAIGN IDENTIFICATION LABEL". EACH LABEL PROVIDES A SPACE TO INCLUDE THE CAMPAIGN NUMBER AND THE FIVE (5) DIGIT DEALER CODE OF THE DEALER PERFORMING THE CAMPAIGN SERVICE. THIS INFORMATION MAY BE INSERTED WITH A TYPEWRITER OR A BALL POINT PEN.

EACH "CAMPAIGN IDENTIFICATION LABEL" IS TO BE LOCATED ON THE RADIATOR CORE SUPPORT IN AN AREA WHICH WILL BE VISIBLE WHEN THE VEHICLE IS BROUGHT IN BY THE CUSTOMER FOR PERIODIC SERVICING. WHEN INSTALLING THE CAMPAIGN IDENTIFICATION LABEL, BE SURE TO PULL THE TAB TO ALLOW ADHESION OF THE CLEAR PROTECTIVE COVERING. ADDITIONAL CAMPAIGN IDENTIFICATION LABELS CAN BE OBTAINED FROM VISPAC INCORPORATED BY CALLING 1-800-269-5100 (MONDAY-FRIDAY, 8:00 A.M. TO 4:30 P.M. EST). ASK FOR ITEM NUMBER S-1015 WHEN ORDERING.

APPLY THE "CAMPAIGN IDENTIFICATION LABEL" ONLY ON A CLEAN, DRY SURFACE.

CLAIM INFORMATION

SUBMIT A PRODUCT CAMPAIGN CLAIM WITH THE INFORMATION INDICATED BELOW:

PART FAILED PARTS LABOR LABOR NET REPAIR PERFORMED COUNT PART NO. ALLOW CC-FC OP * HOURS ITEM

CABLE INSPECTION ONLY 0 N/A N/A MA-96 V0172 0.3

CABLE INSPECTION AND REPLACEMENT 1 12562038 $ 31.92 MA-96 V01730.6

* FOR CAMPAIGN ADMINISTRATIVE ALLOWANCE, ADD 0.1 HOURS TO THE "LABOR HOURS".

** THE "PARTS ALLOWANCE" SHOULD BE THE SUM TOTAL OF THE CURRENT GMSPO DEALER NET PRICE PLUS 40% FOR THE AUTOMATIC TRANSAXLE RANGE SELECTOR CABLE NEEDED TO COMPLETE THE REPAIR.

REFER TO THE GENERAL MOTORS CORPORATION CLAIMS PROCESSING MANUAL FOR DETAILS ON PRODUCT CAMPAIGN CLAIM SUBMISSION.

FIGURES: 24

GM BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THESE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE TOOLS, EQUIPMENT, SAFETY INSTRUCTIONS, AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE YOUR DEALER/RETAILER FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

WE SUPPORT VOLUNTARY TECHNICIAN CERTIFICATION

98023-S

(SAMPLE OF NOTIFICATION USED)

JUNE, 1998

DEAR (CHEVROLET, PONTIAC, OLDSMOBILE) CUSTOMER:

THIS NOTICE IS SENT TO YOU IN ACCORDANCE WITH THE REQUIREMENTS OF THE NATIONAL TRAFFIC AND MOTOR VEHICLE SAFETY ACT.

REASON FOR THIS RECALL: GENERAL MOTORS HAS DECIDED THAT CERTAIN 1998 U-VANS EQUIPPED WITH 3.4L V-6 ENGINES AND AUTOMATIC TRANSMISSIONS FAIL TO CONFORM TO THE FEDERAL MOTOR VEHICLE SAFETY STANDARD 102. THESE VEHICLES MAY HAVE (1) A BROKEN SHIFT CABLE FITTING OR (2) LOOSE SHIFT LINKAGE SWIVEL TUBES. WITH EITHER CONDITION, MOVING THE SHIFT LEVER TO PARK MAY NOT SHIFT THE TRANSMISSION TO PARK. THE VEHICLE COULD ROLL AND A CRASH COULD OCCUR WITHOUT PRIOR WARNING. TO HELP AVOID THIS, WHEN YOU SHIFT TO PARK, ALWAYS APPLY THE PARK BRAKE BEFORE YOU RELEASE THE SERVICE BRAKE.

WHAT WILL BE DONE: YOUR DEALER WILL INSPECT, AND REPLACE IF NECESSARY, THE AUTOMATIC TRANSAXLE RANGE SELECTOR CABLE. THIS SERVICE WILL BE PERFORMED FOR YOU AT NO CHARGE.

HOW LONG WILL THE REPAIR TAKE? THE LENGTH OF TIME REQUIRED TO PERFORM THIS INSPECTION AND/OR SERVICE CORRECTION IS APPROXIMATELY 45 MINUTES. ADDITIONAL TIME MAY BE REQUIRED TO SCHEDULE AND PROCESS YOUR VEHICLE. IF YOUR DEALER HAS A LARGE NUMBER OF VEHICLES AWAITING SERVICE, THIS ADDITIONAL TIME MAY BE SIGNIFICANT. PLEASE ASK YOUR DEALER IF YOU WISH TO KNOW HOW MUCH ADDITIONAL TIME WILL BE NEEDED.

CONTACTING YOUR DEALER: PLEASE CONTACT YOUR DEALER AS SOON AS POSSIBLE TO ARRANGE A SERVICE DATE. PARTS ARE AVAILABLE AND INSTRUCTIONS FOR MAKING THIS CORRECTION HAVE BEEN SENT TO YOUR DEALER. PLEASE ASK YOUR DEALER IF YOU WISH TO KNOW HOW MUCH TIME WILL BE NEEDED TO SCHEDULE, PROCESS AND REPAIR YOUR VEHICLE. YOUR <DIVISION> DEALER IS BEST EQUIPPED TO OBTAIN PARTS AND PROVIDE SERVICES TO CORRECT YOUR VEHICLE AS PROMPTLY AS POSSIBLE. SHOULD YOUR DEALER BE UNABLE TO SCHEDULE A SERVICE DATE WITHIN A REASONABLE TIME, YOU SHOULD CONTACT THE APPROPRIATE CUSTOMER ASSISTANCE/RELATIONS CENTER AT THE LISTED NUMBER BELOW:

DIVISION

NUMBER DEAF, HEARING IMPAIRED OR SPEECH IMPAIRED *

CHEVROLET 1-800-222-1020 1-800-833-2438

PONTIAC 1-800-762-2737 1-800-833-7668

OLDSMOBILE 1-800-442-6537 1-800-833-6537

* UTILIZES TELECOMMUNICATION DEVICES FOR THE DEAF/TEXT TELEPHONES (TDD/TTY)

IF, AFTER CONTACTING THE APPROPRIATE CUSTOMER ASSISTANCE CENTER, YOU ARE STILL NOT SATISFIED THAT WE HAVE DONE OUR BEST TO REMEDY THIS CONDITION WITHOUT CHARGE AND WITHIN A REASONABLE TIME, YOU MAY WISH TO WRITE THE ADMINISTRATOR, NATIONAL HIGHWAY TRAFFIC SAFETY ADMINISTRATION, 400 SEVENTH STREET SW, WASHINGTON, DC 20590 OR CALL 1-800-424-9393 (WASHINGTON, DC RESIDENTS USE 202-366-0123).

CUSTOMER REPLY CARD: THE ENCLOSED CUSTOMER REPLY CARD IDENTIFIES YOUR VEHICLE. PRESENTATION OF THIS CARD TO YOUR DEALER WILL ASSIST IN MAKING THE NECESSARY CORRECTION IN THE SHORTEST POSSIBLE TIME. IF YOU NO LONGER OWN THIS VEHICLE, PLEASE LET US KNOW BY COMPLETING THE POSTAGE PAID REPLY CARD AND RETURNING IT TO US.

WE ARE SORRY TO CAUSE YOU THIS INCONVENIENCE; HOWEVER, WE HAVE TAKEN THIS ACTION IN THE INTEREST OF YOUR SAFETY AND CONTINUED SATISFACTION WITH OUR PRODUCTS.

CHEVROLET, PONTIAC, OLDSMOBILE GENERAL MOTORS CORPORATION

ENCLOSURE

COPYRIGHT 1998 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.

********************************************************************** GM OF CANADA VERSION ********************************************************************** PRODUCT CAMPAIGNS 98023 JUNE 1998

PRODUCT RECALL CAMPAIGN

CMVSS NON-COMPLIANCE CAMPAIGN

#### SUBJECT: CAMPAIGN 98023 SHIFT CABLE RETAINING TABS BREAKING AND SWIVEL TUBE BECOMES DETACHED FROM END FITTING

#### MODELS: 1998 CHEVROLET VENTURE, OLDSMOBILE SILHOUETTE, PONTIAC TRANS SPORT EQUIPPED WITH 3.4L V-6 ENGINE AND AUTOMATIC TRANSMISSION (M13)

DEFECT INVOLVED

GENERAL MOTORS OF CANADA LIMITED HAS DECIDED THAT CERTAIN 1998 U-VANS EQUIPPED WITH 3.4L V-6 (LA1) ENGINES AND AUTOMATIC (M13) TRANSMISSIONS FAIL TO CONFORM TO THE CANADA MOTOR VEHICLE SAFETY STANDARD (CMVSS) 102 "TRANSMISSION SHIFT CONTROL SEQUENCE." THESE VEHICLES MAY HAVE A BROKEN SHIFT CABLE FITTING OR LOOSE SHIFT LINKAGE SWIVEL TUBES. WITH EITHER CONDITION, MOVING THE SHIFT LEVER TO "PARK" MAY NOT SHIFT THE TRANSMISSION TO "PARK". THE VEHICLE COULD ROLL AND A CRASH COULD OCCUR WITHOUT PRIOR WARNING. TO HELP AVOID THIS, THE OPERATOR SHOULD ALWAYS APPLY THE PARK BRAKE BEFORE RELEASING THE SERVICE BRAKE WHEN SHIFTING THE VEHICLE INTO "PARK".

TO CORRECT THIS CONDITION, DEALERS WILL INSPECT AND, IF NECESSARY, REPLACE THE AUTOMATIC SHIFT CABLE.

VEHICLES INVOLVED

INVOLVED ARE CERTAIN 1998 U-VAN MODEL VEHICLES EQUIPPED WITH OPTION CODES LA1 (3.4L V-6 ENGINE) AND M13 (AUTOMATIC TRANSMISSION) AND BUILT WITHIN THE FOLLOWING VIN BREAKPOINTS:

YEAR DIVISION MODEL PLANT CODE FROM THROUGH 1998 ALL U-VAN DORAVILLE "D" WD152963 WD241250

#### NOTE: PLEASE CHECK DCS SCREEN 445 OR YOUR V.I.N. LISTING BEFORE PERFORMING CAMPAIGN TO ENSURE THAT THE VEHICLE IS AFFECTED. ONLY AFFECTED VIN'S WILL BE PAID.

INVOLVED VEHICLES HAVE BEEN IDENTIFIED BY VEHICLE IDENTIFICATION NUMBER. COMPUTER LISTINGS CONTAINING THE COMPLETE VEHICLE IDENTIFICATION NUMBER, CUSTOMER NAME AND ADDRESS DATA HAVE BEEN PREPARED, AND ARE BEING FURNISHED TO INVOLVED DEALERS WITH THE CAMPAIGN BULLETIN. THE CUSTOMER NAME AND ADDRESS DATA FURNISHED WILL ENABLE DEALERS TO FOLLOW-UP WITH CUSTOMERS INVOLVED IN THIS CAMPAIGN. ANY DEALER NOT RECEIVING A COMPUTER LISTING WITH THE CAMPAIGN BULLETIN HAS NO INVOLVED VEHICLES CURRENTLY ASSIGNED.

THESE DEALER LISTINGS MAY CONTAIN CUSTOMER NAMES AND ADDRESSES OBTAINED FROM THE INTER-PROVINCIAL RECORDS. THE USE OF SUCH MOTOR VEHICLE REGISTRATION DATA FOR ANY OTHER PURPOSE IS A VIOLATION OF PROVINCIAL LAWS. ACCORDINGLY, YOU ARE URGED TO LIMIT THE USE OF THIS LISTING TO THE FOLLOW-UP NECESSARY TO COMPLETE THIS CAMPAIGN.

PARTS INFORMATION

#### NOTICE: IT IS ESTIMATED THAT ONLY 10% OF INVOLVED VEHICLES WILL REQUIRE CABLE ASSEMBLY REPLACEMENT. PLEASE ORDER PARTS ACCORDINGLY.

PARTS REQUIRED TO COMPLETE THIS CAMPAIGN ARE TO BE OBTAINED FROM GENERAL MOTORS SERVICE PARTS OPERATIONS (GMSPO). PLEASE REFER TO YOUR "INVOLVED VEHICLES LISTING" PRIOR TO ORDERING REQUIREMENTS.

PART NUMBER DESCRIPTION QUANTITY/VEHICLE 12562038 AUTOMATIC TRANSAXLE SHIFT CABLE ASSEMBLY 1

CUSTOMER NOTIFICATION

ALL CUSTOMERS OF RECORD AT THE TIME OF CAMPAIGN RELEASE ARE SHOWN ON THE ATTACHED COMPUTER LISTING AND HAVE BEEN NOTIFIED BY FIRST CLASS MAIL FROM GENERAL MOTORS (SEE COPY OF CUSTOMER LETTER INCLUDED WITH THIS BULLETIN).

DEALER CAMPAIGN RESPONSIBILITY

ALL UNSOLD NEW VEHICLES IN DEALER'S POSSESSION AND SUBJECT TO THIS CAMPAIGN MUST BE HELD AND INSPECTED/REPAIRED PER THE SERVICE PROCEDURE OF THIS CAMPAIGN BULLETIN BEFORE CUSTOMERS TAKE POSSESSION OF THESE VEHICLES.

DEALERS ARE TO SERVICE ALL VEHICLES SUBJECT TO THIS CAMPAIGN AT NO CHARGE TO CUSTOMERS, REGARDLESS OF MILEAGE, AGE OF VEHICLE, OR OWNERSHIP, FROM THIS TIME FORWARD.

CUSTOMERS WHO HAVE RECENTLY PURCHASED VEHICLES SOLD FROM YOUR VEHICLE INVENTORY, AND FOR WHICH THERE IS NO CUSTOMER INFORMATION INDICATED ON THE DEALER LISTING, ARE TO BE CONTACTED BY THE DEALER. ARRANGEMENTS ARE TO BE MADE TO MAKE THE REQUIRED CORRECTION ACCORDING TO THE INSTRUCTIONS CONTAINED IN THIS BULLETIN. THIS COULD BE DONE BY MAILING TO SUCH CUSTOMERS A COPY OF THE APPROPRIATE CUSTOMER LETTER ACCOMPANYING THIS BULLETIN.

IN SUMMARY, WHENEVER A VEHICLE SUBJECT TO THIS CAMPAIGN ENTERS YOUR VEHICLE INVENTORY, OR IS IN YOUR DEALERSHIP FOR SERVICE IN THE FUTURE, YOU MUST TAKE THE STEPS NECESSARY TO BE SURE THE CAMPAIGN CORRECTION HAS BEEN MADE BEFORE SELLING OR RELEASING THE VEHICLE.

SERVICE PROCEDURE

THE CAMPAIGN SERVICE PROCEDURE INVOLVES INSPECTION OF THE AUTOMATIC TRANSAXLE RANGE SELECTOR CABLE, THEN IF NECESSARY, REPLACEMENT OF THE SHIFT CABLE.

INSPECTION PROCEDURE - ALL VEHICLES

1. SET THE PARKING BRAKE.

2. BLOCK THE WHEELS

3. REMOVE PUSH-IN RETAINERS FROM DRIVER SIDE INSTRUMENT PANEL INSULATOR TO INSTRUMENT PANEL.

4. REMOVE PRESS-ON RETAINERS FROM DRIVER SIDE INSTRUMENT PANEL INSULATOR TO DASH MAT.

5. REMOVE INSTRUMENT PANEL COURTESY LAMP BY UNSNAPPING FROM INSTRUMENT PANEL INSULATOR.

6. REMOVE INSTRUMENT PANEL INSULATOR FROM INSTRUMENT PANEL.

7. REMOVE BOLTS/SCREWS FROM BOTTOM OF KNEE BOLSTER.

8. REMOVE KNEE BOLSTER BY PULLING TO RELEASE UPPER CLIPS.

9. SHIFT THE STEERING COLUMN TRANSMISSION SHIFT LEVER INTO THE LOW GEAR (L1) POSITION.

#### NOTE: THE VEHICLE DOES NOT HAVE TO BE STARTED OR RUNNING, BUT THE IGNITION KEY MUST BE IN THE "ACCESSORY" OR IN THE "ON" POSITION IN ORDER TO MOVE THE STEERING COLUMN TRANSMISSION SHIFT LEVER.

10. INSPECT SWIVEL TUBE RETENTION BY PULLING THE BLACK PLASTIC TUBE UPWARDS TOWARDS THE STEERING WHEEL.

#### NOTE: EXCESSIVE FORCE IS NOT REQUIRED TO VERIFY PROPER RETENTION OF THE TUBE TO THE CABLE CONDUIT FITTING. IF THE SWIVEL TUBE IS NOT PROPERLY SEATED IT CAN BE DISLODGED WITH A RELATIVELY LIGHT AXIAL FORCE [cent ]LESS THAN 80 N (20 LBS.)|. THIS CAN BE ACCOMPLISHED BY USING TWO OR THREE FINGERS TO PULL UPWARDS ON THE TUBE TO VERIFY RETENTION.

11. VISUALLY INSPECT FOR BROKEN, CRACKED, OR MISSING RETAINING TABS ON THE SHIFT CABLE CONDUIT FITTING AT THE STEERING COLUMN BRACKET.

12. INSPECT FOR PRESENCE OF THE CABLE RETAINER THAT HOLDS THE PLASTIC TABS OF THE CABLE FITTING AGAINST THE BRACKET. THE CABLE RETAINER IS SHAPED LIKE A LARGE STAPLE.

13. IF UPON INSPECTION, THE SWIVEL TUBE CAN BE DISLODGED OR BECOMES DISCONNECTED, OR THE RETAINING TABS ARE CRACKED OR MISSING, OR THE CABLE RETAINER IS MISSING, THE SHIFT CABLE MUST BE REPLACED. FOLLOW THE AUTOMATIC TRANSAXLE RANGE SELECTOR CABLE REMOVAL, INSTALLATION, AND ADJUSTMENT PROCEDURE STARTING WITH STEP 25. OTHERWISE, CONTINUE WITH STEP 14 TO REINSTALL THE KNEE BOLSTER AND THE INSTRUMENT PANEL INSULATOR.

#### NOTICE: REFER TO FASTENER NOTICE IN CAUTIONS AND NOTICES.

14. SHIFT THE STEERING COLUMN TRANSMISSION SHIFT LEVER INTO THE "PARK" POSITION.

15. TURN IGNITION KEY TO THE "OFF" POSITION.

16. INSTALL KNEE BOLSTER TO INSTRUMENT PANEL BY LOCATING CLIPS TO SLOTS INSTRUMENT PANEL AND PUSHING TO SECURE.

17. INSTALL BOLTS/SCREWS TO BOTTOM OF KNEE BOLSTER. TIGHTEN BOLTS/SCREWS TO 2.5 N M (22 LB. IN.)

18. INSTALL INSTRUMENT PANEL COURTESY LAMP BY SNAPPING INTO INSTRUMENT PANEL INSULATOR.

19. POSITION INSTRUMENT PANEL INSULATOR TO INSTRUMENT PANEL.

20. INSTALL PRESS-ON RETAINERS TO INSTRUMENT PANEL INSULATOR TO DASH MAT.

21. INSTALL PUSH-IN RETAINERS TO INSTRUMENT PANEL INSULATOR TO INSTRUMENT PANEL.

22. UNBLOCK WHEELS.

23. RELEASE THE PARKING BRAKE WHILE APPLYING THE SERVICE BRAKE.

24. INSTALL CAMPAIGN IDENTIFICATION LABEL.

AUTOMATIC TRANSAXLE RANGE SELECTOR CABLE REMOVAL, INSTALLATION, AND ADJUSTMENT

REMOVAL

25. REMOVE THE THROTTLE BODY AIR INLET DUCT.

26. REMOVE THE AUTOMATIC TRANSAXLE RANGE SELECTOR CABLE FROM THE AUTOMATIC TRANSAXLE RANGE SELECTOR MANUAL LEVER.

27. REMOVE RETAINER FROM THE AUTOMATIC TRANSAXLE RANGE SELECTOR CABLE.

28. REMOVE THE AUTOMATIC TRANSAXLE RANGE SELECTOR CABLE FROM THE AUTOMATIC TRANSAXLE RANGE SELECTOR CABLE BRACKET.

29. REMOVE THE DRIVER SIDE INSTRUMENT PANEL INSULATOR, IF NOT ALREADY REMOVED DURING INSPECTION PROCEDURE (SEE PROCEDURE STEPS 3 - 8 ON PAGES 3 AND 4).

30. REMOVE THE KNEE BOLSTER, IF NOT ALREADY REMOVED DURING INSPECTION PROCEDURE (SEE PROCEDURE STEPS 3 - 8 ON PAGES 3 AND 4).

31. REMOVE THE AUTOMATIC TRANSAXLE RANGE SELECTOR CABLE FROM THE COLUMN CONTROL LEVER BALL STUD.

32. REMOVE CABLE RETAINER FROM AUTOMATIC TRANSAXLE RANGE SELECTOR CABLE.

33. REMOVE THE AUTOMATIC TRANSAXLE RANGE SELECTOR CABLE FROM THE STEERING COLUMN BRACKET.

34. REMOVE THE AUTOMATIC TRANSAXLE RANGE SELECTOR CABLE THROUGH THE HOLE IN THE COWL.

INSTALLATION

35. PROPERLY ROUTE THE NEW AUTOMATIC TRANSAXLE RANGE SELECTOR CABLE THROUGH THE ENGINE COMPARTMENT.

36. PROPERLY ROUTE THE AUTOMATIC TRANSAXLE RANGE SELECTOR CABLE THROUGH THE COWL.

37. INSTALL THE AUTOMATIC TRANSAXLE RANGE SELECTOR CABLE TO THE STEERING COLUMN BRACKET.

38. INSTALL CABLE RETAINER TO THE CABLE FITTING AGAINST THE STEERING COLUMN BRACKET.

39. INSTALL THE AUTOMATIC TRANSAXLE RANGE SELECTOR CABLE TO THE COLUMN CONTROL LEVER BALL STUD.

40. INSTALL THE AUTOMATIC TRANSAXLE RANGE SELECTOR CABLE TO THE AUTOMATIC TRANSAXLE RANGE SELECTOR CABLE BRACKET.

41. INSTALL THE CABLE RETAINER TO THE CABLE ADJUSTER FITTING AGAINST THE AUTOMATIC TRANSAXLE RANGE SELECTOR CABLE BRACKET.

42. INSTALL THE AUTOMATIC TRANSAXLE RANGE SELECTOR CABLE TO THE AUTOMATIC TRANSAXLE RANGE SELECTOR LEVER BALL STUD.

CABLE ADJUSTMENT

#### NOTICE: ADJUST THE AUTOMATIC TRANSAXLE RANGE SELECTOR CABLE WHILE THE TRANSAXLE AND THE GEAR SELECTOR ARE IN THE "NEUTRAL" POSITION ONLY. FAILURE TO DO SO MAY CAUSE MIS- ADJUSTMENT.

43. USE APPROPRIATE TOOL TO PRY ON THE AUTOMATIC TRANSAXLE RANGE SELECTOR CABLE TERMINAL AT THE AUTOMATIC TRANSAXLE RANGE SELECTOR LEVER TO REMOVE THE AUTOMATIC TRANSAXLE RANGE SELECTOR CABLE TERMINAL FROM THE TRANSAXLE MANUAL SHAFT LEVER PIN.

#### NOTICE: DO NOT PRY AND DO NOT PULL UP ON ANY OTHER PART OF THE AUTOMATIC TRANSAXLE RANGE SELECTOR CABLE OR DAMAGE MAY OCCUR.

44. FULLY LIFT UP THE ADJUSTER LOCK BUTTON. ENSURE THE ADJUSTER IS FREE TO MOVE.

ADJUSTER IS NEXT TO THE CABLE RETAINER LOCATED AT THE TRANSAXLE SIDE OF THE AUTOMATIC TRANSAXLE RANGE SELECTOR CABLE.

45. ROTATE THE AUTOMATIC TRANSAXLE RANGE SELECTOR MANUAL LEVER (LOCATED AT THE TRANSAXLE) FULLY COUNTERCLOCKWISE TO THE "PARK" GEAR POSITION, THEN ROTATE THE LEVER CLOCKWISE TWO (2) CLICKS INTO THE "NEUTRAL" GEAR TO PLACE THE AUTOMATIC TRANSAXLE RANGE SELECTOR MANUAL LEVER IN THE "NEUTRAL" GEAR POSITION.

46. PERFORM THE FOLLOWING STEPS TO PLACE THE STEERING COLUMN SHIFTER LEVER INTO THE "NEUTRAL" POSITION:

(A) ROTATE THE SHIFT LEVER TO THE "LOW 1" (L1) POSITION, FULLY DOWN.

(B) PUSH FORWARD ON THE LEVER WHILE SLOWLY PUSHING UP. THE GEAR SHIFT LEVER WILL MOVE UP WHILE CLICKING OVER THE GEAR OVER TRAVEL STOPS.

(C) RELEASE THE GEAR SHIFT ONCE THE GEAR SHIFT LEVER STOPS SOLIDLY. THE GEAR SHIFT LEVER IS NOW IN THE "NEUTRAL" POSITION.

47. GRASP THE AUTOMATIC TRANSAXLE RANGE SELECTOR CABLE TERMINAL IN THE UNDERHOOD AREA.

48. PULL THE AUTOMATIC TRANSAXLE RANGE SELECTOR CABLE TERMINAL TOWARDS THE BALL STUD ON THE AUTOMATIC TRANSAXLE RANGE SELECTOR MANUAL LEVER. THE TRANSAXLE RANGE SELECTOR CABLE ADJUSTER SPRING SHOULD COMPRESS AS THE TERMINAL IS MOVED TOWARD THE PIN.

49. CAREFULLY PUSH DOWN ON THE TERMINAL UNTIL THE TERMINAL SNAPS TO ATTACH THE TERMINAL TO THE AUTOMATIC TRANSAXLE RANGE SELECTOR MANUAL LEVER BALL STUD.

DO NOT MOVE THE AUTOMATIC TRANSAXLE RANGE SELECTOR MANUAL LEVER OUT OF POSITION WHILE PERFORMING THIS PROCEDURE.

DO NOT PULL THE TERMINAL BEYOND THE PIN THEN PUSH BACK OR THE STEERING COLUMN SHIFTER MAY MOVE OUT OF THE "NEUTRAL" POSITION.

50. PRESS THE ADJUSTER LOCK BUTTON DOWN FLUSH WITH THE ADJUSTER BODY.

51. SHIFT TO "PARK".

52. UNBLOCK WHEELS.

53. RELEASE THE PARKING BRAKE WHILE APPLYING THE SERVICE BRAKE.

54. START THE ENGINE.

55. ENSURE ALL THE INDICATED GEAR POSITIONS MATCH THE VEHICLE RESPONSE.

56. SHIFT TRANSAXLE TO "PARK".

57. TURN THE IGNITION KEY TO THE "OFF" POSITION.

58. INSTALL THE THROTTLE BODY AIR INLET DUCT.

#### NOTICE: REFER TO FASTENER NOTICE IN CAUTIONS AND NOTICES.

59. INSTALL KNEE BOLSTER TO INSTRUMENT PANEL BY LOCATING CLIPS TO SLOTS INSTRUMENT PANEL AND PUSHING TO SECURE.

60. INSTALL BOLTS/SCREWS TO BOTTOM OF KNEE BOLSTER. TIGHTEN BOLTS/SCREWS TO 2.5 N M (22 LB. IN.)

61. INSTALL INSTRUMENT PANEL COURTESY LAMP BY SNAPPING INTO INSTRUMENT PANEL INSULATOR.

62. POSITION INSTRUMENT PANEL INSULATOR TO INSTRUMENT PANEL.

63. INSTALL PRESS-ON RETAINERS TO INSTRUMENT PANEL INSULATOR TO DASH MAT.

64. INSTALL PUSH-IN RETAINERS TO INSTRUMENT PANEL INSULATOR TO INSTRUMENT PANEL.

65. INSTALL CAMPAIGN IDENTIFICATION LABEL

CAMPAIGN IDENTIFICATION LABEL

EACH VEHICLE CORRECTED IN ACCORDANCE WITH THE INSTRUCTIONS OUTLINED IN THIS PRODUCT CAMPAIGN BULLETIN WILL REQUIRE A "CAMPAIGN IDENTIFICATION LABEL." EACH LABEL PROVIDES A SPACE TO INCLUDE THE CAMPAIGN NUMBER AND THE FIVE (5) DIGIT DEALER CODE OF THE DEALER PERFORMING THE CAMPAIGN SERVICE. THIS INFORMATION MAY BE INSERTED WITH A TYPEWRITER OR A BALL POINT PEN.

INSERT CAMPAIGN NUMBER

INSERT DEALER CODE

EACH "CAMPAIGN IDENTIFICATION LABEL" IS TO BE LOCATED ON THE RADIATOR CORE SUPPORT IN AN AREA WHICH WILL BE VISIBLE WHEN THE VEHICLE IS BROUGHT IN BY THE CUSTOMER FOR PERIODIC SERVICING. ADDITIONAL CAMPAIGN IDENTIFICATION LABELS CAN BE OBTAINED FROM DGN BY CALLING 1-800-668-5539 (MONDAY-FRIDAY, 8:00 A.M. TO 5:00 P.M. EST). ASK FOR ITEM NUMBER GMP 91 WHEN ORDERING.

APPLY THE "CAMPAIGN IDENTIFICATION LABEL" ONLY ON A CLEAN, DRY SURFACE.

CLAIM INFORMATION

SUBMIT A PRODUCT CAMPAIGN CLAIM WITH THE INFORMATION INDICATED BELOW:

PART FAILED PARTS LABOR LABOR NET REPAIR PERFORMED COUNT PART NO. ALLOW CC-FC OP * HOURS ITEM CABLE INSPECTION ONLY -- -- -- MA-96 V0172 0.3

CABLE INSPECTION AND REPLACEMENT 1 12562038 ** MA-96 V0173 0.6

* FOR CAMPAIGN ADMINISTRATIVE ALLOWANCE, ADD 0.1 HOURS TO THE "LABOUR HOURS".

** THE "PARTS ALLOWANCE" SHOULD BE THE SUM TOTAL OF THE CURRENT GMSPO DEALER NET PRICE PLUS 40% FOR THE AUTOMATIC TRANSAXLE RANGE SELECTOR CABLE NEEDED TO COMPLETE THE REPAIR.

REFER TO THE GENERAL MOTORS CLAIMS PROCESSING MANUAL FOR DETAILS ON PRODUCT CAMPAIGN CLAIM SUBMISSION.

GM BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THESE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE TOOLS, EQUIPMENT, SAFETY INSTRUCTIONS, AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE YOUR DEALER/RETAILER FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

WE SUPPORT VOLUNTARY TECHNICIAN CERTIFICATION

COPYRIGHT 1998 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.