For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Was the entire HVAC System Check performed? | -- | Go to Step 2 | Go to HVAC System Check
2 |

1. Turn the ignition switch to the RUN position.
2. Turn both rear blower switches to the OFF position.
3. Disconnect the rear window wiper/washer and multi-function switch connector C2.

Does the rear blower turn off?

--

Go to Step 3

Go to Step 4

3 | Replace the rear window wiper/washer and multi-function switch. Refer to Auxiliary Air Conditioning (A/C) Control Assembly Replacement - Front . Is the repair complete? | -- | Go to Step 5 | --
4 | Repair a short to B+ in circuit 1176, 1072, or 1052. Is the repair complete? | -- | Go to Step 5 | --
5 |

1. Turn the ignition switch to the OFF position.
2. Reconnect all connectors /components removed.

Have all the repairs been made?

--

Go to HVAC System Check

--