For 1990-2009 cars

### Removal Procedure

1. Remove the rear quarter window. Refer to Quarter Window Replacement .
2. Pull the rear quarter window weather strip from the pinch-weld flange
3. Remove the rear quarter window weather-strip from the vehicle.

### Installation Procedure

Important: The rear quarter window weather-strip service replacement part is a cut-to-fit part. The weather-strip must be trimmed to fit the window opening and joined together.

1. Install the rear quarter window weather-strip to the vehicle.
2. Align the rear quarter window weather-strip joint to center of the rear quarter window latch attachment point.
3. Roll the rear quarter window weather-strip from joint to bottom of window to ensure a proper seal.
4. Install the rear quarter window. Refer to Quarter Window Replacement .