For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
Auto Level Control (ALC) Air Compressor | Under the vehicle, behind the LR wheelhouse | Automatic Level Control Suspension Component Views | Automatic Level Control Suspension Connector End Views
Auto Level Control (ALC) Inflator Relay | In the vehicle, behind the left rear wheelhouse | Automatic Level Control Suspension Component Views | Automatic Level Control Suspension Connector End Views
Auto Level Control (ALC) Inflator Solenoid Valve | Behind the left rear wheelhouse | Automatic Level Control Suspension Component Views | --
Auto Level Control (ALC) Sensor | Mounted to the rear crossmember above the rear axle | Automatic Level Control Suspension Component Views | Automatic Level Control Suspension Connector End Views
Fuse Block | Right side of the IP, in the right front door opening | Power and Grounding Component Views | --
Inflator Air Switch | Behind the left rear wheelhouse | Automatic Level Control Suspension Component Views | Automatic Level Control Suspension Connector End Views
C200 (56 cavities) | IP wiring harness to the right side of the body wiring harness, behind the right side of the IP compartment, below P100 | Harness Routing Views | Inline Harness Connector End Views
C203 (56 cavities) | IP wiring harness to the left side of the body wiring harness, left side of the steering column, below P101 | Harness Routing Views | Inline Harness Connector End Views
C405 (10 cavities) | Body wiring harness to the auto level control wiring harness, behind the left quarter panel, behind the left rear wheelhouse | Harness Routing Views | Inline Harness Connector End Views
C407 (6 cavities) | Auto level control wiring harness to the trailer rear wiring harness, beneath the vehicle, near P403, near the left rear wheelhouse | Harness Routing Views | Inline Harness Connector End Views
G401 | Secured to the lower left D-pillar | Harness Routing Views | --
P403 | Behind the left wheelhouse | Harness Routing Views | --
S209 | IP harness, center of the IP approximately 8 cm (3 in) from the security indicator lamp breakout | -- | --
S337 | Body harness, rear of the left B-pillar base approximately 8 cm (3 in) from the P401 breakout | -- | --
S441 | Auto level control harness, left rear of the body approximately 24 cm (9 in) from P403 | -- | --
S443 | Auto level control harness, left rear of the body approximately 20 cm (8 in) from P403 | -- | --
S445 | Auto level control harness, left rear of the body approximately 16 cm (6 in) from P403 | -- | --