For 1990-2009 cars

### Removal Procedure

1. Remove the liftgate. Refer to Liftgate Replacement .
2. Remove the headliner. Refer to Headlining Trim Panel Replacement in Interior Trim.
3. Use a grease pencil to mark the liftgate hinge position to the body.
4. Remove the hinge retaining nuts from the vehicle roof.
5. Remove the hinge from the vehicle.

### Installation Procedure

1. Align the hinge with the marks made on the vehicle body.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the hinge retaining nuts.

Tighten
Tighten the nuts to 25 N·m (18 lb ft).

3. Install the headliner. Refer to Headlining Trim Panel Replacement in Interior Trim.
4. Install the liftgate. Refer to Liftgate Replacement .