For 1990-2009 cars

Table 1: | Cigar Lighter Connector
Table 2: | Front Electric Accessory Plug Housing
Table 3: | Rear Electric Accessory Plug Housing
Table 4: | Underhood Accessory Wiring Junction Block C1
Table 5: | Underhood Accessory Wiring Junction Block C2
Table 6: | Underhood Accessory Wiring Junction Block C3
Table 7: | Underhood Accessory Wiring Junction Block C4
Table 8: | Underhood Accessory Wiring Junction Block C5
Table 9: | Underhood Accessory Wiring Junction Block C6

#### Cigar Lighter Connector

Connector Part Information |

• | 12047699

• | 1 M Sleeve & 1 C/LTR P2S (Gray)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | ORN | 440 | Fused ignition feed
B | BLK | 1450 | Ground

#### Front Electric Accessory Plug Housing

Connector Part Information |

• | 12033934

• | 2-Way 56 Series Lock Type (Gray)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | ORN | 1940 | Fused ignition feed
B | BLK | 150 | Ground

#### Rear Electric Accessory Plug Housing

Connector Part Information |

• | 12033934

• | 2-Way F 56 Series (Gray)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | ORN | 2540 | Fused ignition feed
B | BLK | 850 | Ground

#### Underhood Accessory Wiring Junction Block C1

Connector Part Information |

• | 15303513

• | 68-Way F Metri-Pack 280 Series Flexlock (Black)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A1-A4 | -- | -- | Not Used
A5 | DK GRN/ORN | 465 | Fuel pump relay feed-coil
A6-A7 | -- | -- | Not Used
A8 | ORN | 840 | Fused battery feed
A9 | PNK | 339 | Fused ignition 1 feed
A10 | DK BLU | 532 | Engine coolant fan 1 (right) motor feed-secondary
A11 | -- | -- | Not Used
A12 | PNK | 639 | Fused ignition 1 feed
B1-B2 | -- | -- | Not Used
B3 | DK GRN | 135 | Engine coolant temperature sensor
B4 | RED | 490 | Fuel pump relay feed-N.C. contact-prime
B5-B6 | -- | -- | Not Used
B7 | PNK | 1339 | Fused ignition 1 feed
B8 | -- | -- | Not Used
B9 | PNK | 339 | Fused ignition 1 feed
B10 | BRN/WHT | 419 | Check engine indicator lamp output
B11-B12 | -- | -- | Not Used
C1 | BRN/WHT | 1173 | Low oil level indicator lamp output
C2-C5 | -- | -- | Not Used
C8 | -- | -- | Not Used
C9 | PNK | 339 | Fused ignition 1 feed
C10 | DK BLU | 473 | Engine coolant fan 2 (left) relay output-coil
C11 | BLK | 1050 | Ground
C12 | -- | -- | Not Used
D1 | YEL | 772 | Transaxle range switch input B
D2 | -- | -- | Not Used
D3 | BLK/WHT | 451 | PCM ground
D4 | -- | -- | Not Used
D5 | BLK/WHT | 451 | PCM ground
D8 | -- | -- | Not Used
D9 | PNK | 339 | Fused ignition 1 feed
D10 | DK GRN | 83 | Cruise control signal-disengage
D11 | PNK | 439 | Fused ignition 1 feed
D12 | TAN | 31 | Oil pressure indicator lamp output
E1 | GRY | 773 | Transaxle range switch input C
E2 | ORN | 540 | Fused battery feed
E3 | PPL | 420 | Brake pedal switch output-torque converter clutch
E4 | LT GRN | 275 | Transaxle range switch feed-PARK
E5 | DK GRN | 389 | Vehicle speed signal
E6 | DK GRN | 35 | Coolant temperature indicator lamp output
E7-E11 | -- | -- | Not Used
E12 | ORN | 2740 | Fused battery feed
F1 | WHT | 776 | Transaxle range switch parity input
F2 | WHT | 504 | Engine coolant fan 1 (right) motor output
F3 | DK GRN | 335 | Coolant fan 1 relay output-coil
F4 | WHT | 85 | Cruise control indicator lamp output
F5 | BRN | 25 | Charge indicator lamp
F6 | WHT | 121 | Tachometer signal
F7 | DK GRN/WHT | 459 | A/C CLU relay output coil
F8 | DK GRN | 59 | A/C compressor clutch coil solenoid feed
F9 | PNK | 239 | Fused ignition 1 feed
F10 | LT GRN/BLK | 24 | Backup lamp feed
F11 | LT BLU | 409 | Engine coolant fan 2 (left) feed
F12 | BLK/WHT | 771 | Transaxle range switch input A

#### Underhood Accessory Wiring Junction Block C2

Connector Part Information |

• | 15303514

• | 68-Way F Metri-Pack 280 Series Flexlock (Brown)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A1 | WHT | 776 | Transaxle range switch parity input
A2-A3 | -- | -- | Not Used
A4 | WHT | 85 | Cruise control indicator lamp output
A5 | BRN | 25 | Charge indicator lamp
A6 | WHT | 121 | Tachometer signal
A7-A9 | -- | -- | Not Used
A10 | LT GRN/BLK | 24 | Backup lamp feed
A11 | -- | -- | Not Used
A12 | BLK/WHT | 771 | Transaxle range switch input A
B1 | GRY | 773 | Transaxle range switch input C
B2-B4 | -- | -- | Not Used
B5 | GRY | 120 | Fuel pump motor feed
B6 | DK GRN | 35 | Coolant temperature indicator lamp output
B7-B9 | -- | -- | Not Used
B10 | DK GRN | 83 | Cruise control signal-disengage
B11-B12 | -- | -- | Not Used
C1 | -- | -- | Not Used
C2 | YEL | 772 | Transaxle range switch input B
C3 | PPL | 420 | Brake pedal switch output-torque converter clutch
C4 | LT GRN | 275 | Transaxle range switch feed-PARK
C5 | -- | -- | Not Used
C8 | DK GRN | 389 | Vehicle speed signal
C9 | -- | -- | Not Used
C10 | PNK | 439 | Fused ignition 1 feed
C11-C12 | -- | -- | Not Used
D1 | ORN | 1340 | Fused battery feed
D2 | -- | -- | Not Used
D3 | DK GRN | 135 | Engine coolant temperature sensor
D4 | LT GRN | 275 | Transaxle range switch feed-PARK
D5 | PNK | 1339 | Fused ignition 1 feed
D8 | DK GRN | 389 | Vehicle speed signal
D9 | -- | -- | Not Used
D10 | BRN/WHT | 419 | Check engine indicator lamp output
D11 | TAN | 31 | Oil pressure indicator lamp output
D12 | -- | -- | Not Used
E1 | ORN | 1340 | Fused battery feed
E2 | -- | -- | Not Used
E3 | YEL/BLK | 68 | Low coolant warning indicator lamp output
E4 | -- | -- | Not Used
E5 | YEL | 317 | Fog lamp relay feed-coil
E6 | -- | -- | Not Used
E7 | BLK | 28 | Horn relay output-coil
E8 | DK GRN | 389 | Vehicle speed signal
E9-E10 | -- | -- | Not Used
E11 | YEL | 18 | Tail/turn/stop lamp feed-left rear
E12 | -- | -- | Not Used
F1-F2 | -- | -- | Not Used
F3 | BRN/WHT | 1173 | Low oil level indicator lamp output
F4 | LT GRN | 11 | High beam headlamp feed
F5 | PPL | 34 | Fog lamp indicator feed
F6 | -- | -- | Not Used
F7 | ORN | 640 | Fused battery feed
F8 | TAN | 12 | Low beam headlamp feed
F9 | LT BLU | 14 | Turn signal lamp feed-left front
F10 | DK BLU | 15 | Turn signal lamp feed-right front
F11 | BRN | 9 | Park lamp feed
F12 | DK GRN | 19 | Tail/stop/stop lamp feed-right rear

#### Underhood Accessory Wiring Junction Block C3

Connector Part Information |

• | 15303512

• | 68-Way F Metri-Pack 280 Series Flexlock (Gray)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A1-A3 | -- | -- | Not Used
A4 | LT GRN | 11 | High beam headlamp feed
A5 | PPL | 34 | LH Fog lamp feed
A6 | -- | -- | Not Used
A7 | DK GRN | 29 | Horn feed
A8 | TAN | 12 | Low beam headlamp feed
A9 | LT BLU | 14 | Turn signal lamp feed-left front
A10 | DK BLU | 15 | Turn signal lamp feed-right front
A11 | BRN | 9 | Park lamp feed
A12 | DK GRN | 19 | Tail/turn stop lamp feed-right rear
B1-B3 | -- | -- | Not Used
B4 | LT GRN | 11 | High beam headlamp feed
B5 | PPL | 34 | RH Fog lamp feed
B6 | -- | -- | Not Used
B7 | DK GRN | 29 | Horn feed
B8-B10 | -- | -- | Not Used
B11 | BRN | 9 | Park lamp feed
B12 | -- | -- | Not Used
C1-C5 | -- | -- | Not Used
C8-C10 | -- | -- | Not Used
C11 | BRN | 9 | Park lamp feed
C12 | -- | -- | Not Used
D1-D5 | -- | -- | Not Used
D8D10 | -- | -- | Not Used
D11 | BRN | 9 | Park lamp feed
D12 | -- | -- | Not Used
E1-E10 | -- | -- | Not Used
E11 | YEL | 18 | Tail/turn/stop lamp feed-left rear
E12 | -- | -- | Not Used
F1-F12 | -- | -- | Not Used

#### Underhood Accessory Wiring Junction Block C4

Connector Part Information |

• | 12146038

• | 2-Way F MaxiFuse (Gray)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | RED | 242 | Fused battery feed
B | RED | 142 | Fused battery feed

#### Underhood Accessory Wiring Junction Block C5

Connector Part Information |

• | 12146037

• | 2-Way F MaxiFuse (Black)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | -- | -- | Not Used
B | RED | 42 | Fused battery feed

#### Underhood Accessory Wiring Junction Block C6

Connector Part Information |

• | 12160605

• | 2-Way F MaxiFuse (Green)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | RED | 642 | Fused battery feed
B | RED | 742 | Fused battery feed