For 1990-2009 cars

## Valve Rocker Arm Cover Removal Left Side

1. Remove the spark plug wires.
2. Remove the electronic ignition control module nuts and bolts.
3. Remove the electronic ignition control module.
4. Disconnect the vacuum lines from the upper intake manifold.
5. Remove the valve rocker arm cover bolts.
6. Remove the valve rocker arm cover and gasket.

## Valve Rocker Arm Cover Removal Right Side

1. Remove the valve rocker arm cover bolts.
2. Remove the valve rocker arm cover and gasket.