For 1990-2009 cars

### Removal Procedure

#### Tools Required

J 38778 Door Trim Pad and Garnish Clip Remover

1. Open and suitably support the hood.
2. Use J 38778 in order to remove the push-in retainers from the hood front seal.
3. Remove the hood front seal from the hood.

### Installation Procedure

Important: Install the grille prior to the hood front seal.

1. Install the hood front seal to the hood.
2. Install the push-in retainers to the hood front seal.
3. Close the hood.