For 1990-2009 cars

### Removal Procedure

1. Remove the instrument panel (I/P) compartment.

1.1. | Open the I/P compartment door.

1.2. | Remove the 4 bolts (1).

1.3. | Disconnect the wiring harness plug.

1.4. | Remove the I/P compartment.

2. Remove the I/P compartment door damper.

2.1. | Release the fastening clip (1).

2.2. | Remove the damper.

### Installation Procedure

1. Install the I/P compartment.

Install the fastening clamp.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the I/P compartment.

2.1. | Connect the wiring harness plug.

2.2. | Insert the I/P compartment.

Tighten
Tighten the 4 bolts to 4 N·m (35 lb in).

2.3. | Close the I/P compartment door.