For 1990-2009 cars

1. Clean the sealing surfaces.
2. Inspect for plane surface.

• | Cylinder block, cylinder head

• | Straight-edge, feeler gauge

3. Install the cylinder head gasket.
4. Install the cylinder head.

Caution: Refer to Fastener Caution in the Preface section.

Note: Note the correct tightening sequence.

5. Install NEW cylinder head bolts. Tighten the 10 bolts to 25 N·m (18 lb ft) + 90 degrees + 45 degrees.