For 1990-2009 cars

#### Special Tools

KM-6004-2 Tie Rod Wrench

### Removal Procedure

1. Remove the corresponding tie rod end from the tie rod. Refer to Steering Linkage Outer Tie Rod Replacement .

Important: To remove and refit the right-hand tie rod the left-hand boot must also be detached from the steering gear. A flat surface is to be found on the steering shaft side to hold against the steering rack (arrows).

2. Remove the corresponding boot. Refer to Rack and Pinion Boot Replacement .
3. Remove the tie rod with KM-6004-2 (1) from the steering rack.

Counterhold with an open-ended wrench (2) on the toothed rack flat.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the tie rod outer linkage to the steering gear.

Tighten
Tighten to 90 N·m (67 lb ft).

• | Clean the rack thread and coat with locking compound.

• | Install the tie rod to the rack with KM-6004-2 (1).

• | Counterhold with an open-ended wrench (2) on the toothed rack flat (arrow).

2. Install the boot or boots. Refer to Rack and Pinion Boot Replacement .
3. Install the corresponding tie rod end. Refer to Steering Linkage Outer Tie Rod Replacement .
4. Inspect the straight-ahead position, adjust if necessary. Refer to Straight Ahead Inspection .
5. Inspect the toe-in, adjust if necessary. Refer to Front Toe Adjustment .