For 1990-2009 cars

## Antenna Cable Replacement Coupe

#### Special Tools

KM6067 Radio Removal Tools

### Removal Procedure

Important: Replace or repair wiring harnesses observing the safety regulations of electrics/electronics.

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the battery.
2. Remove the radio.

• | Install the removal bar KM6067 into the openings (arrows) until it engages.

• | Pull both removal bars outwards and at the same time withdraw the radio from the holder.

3. Disconnect the wiring harness plug.

Disconnect the 2 wiring harness plugs (1, 2).

4. Remove the instrument panel (I/P) compartment.

• | Open the I/P compartment door.

• | Remove the 4 bolts (1).

• | Disconnect the wiring harness plug.

• | Remove the I/P compartment.

5. Remove the door sill inner panel.

• | Release the 5 clips.

• | Remove the sill inner panel (1).

6. Lower the headlining trim panel. Refer to Headlining Trim Panel Replacement .
7. Remove the rear compartment side trim panel. Refer to Rear Compartment Side Trim Panel Replacement .
8. Disconnect the roof antenna wiring harness plug (1).
9. Disconnect the antenna cable (1) and insulate the remaining ends.

Important:

• | The old antenna cable remains in the wiring harness.

• | The new antenna cable is routed parallel to the existing antenna cable and is secured with duct tape and cable ties.

10. Route the antenna cable up to behind the I/P compartment.
11. Disconnect the antenna cable from I/P padding wiring harness.

Disconnect and insulate the wiring harness (1).

### Installation Procedure

1. Connect the wiring harness plug of the roof aerial.
2. Install headlining trim panel. Refer to Headlining Trim Panel Replacement .
3. Remove the rear compartment side trim panel. Refer to Rear Compartment Side Trim Panel Replacement .
4. Install the radio.

• | Connect the 2 wiring harness plugs.

• | Push the radio into the holder until it engages.

5. Install the I/P compartment.

Connect the wiring harness plug.

Notice: Refer to Fastener Notice in the Preface section.

6. Install the I/P compartment.

Tighten
Tighten the 4 screws to 4 N·m (35 lb in).

Close the I/P compartment door.

7. Install the door sill inner panel.

Clip in the 5 clips.

8. Connect the battery.
9. For reprogramming procedures, refer to Control Module References .

## Antenna Cable Replacement Sedan

#### Special Tools

KM6067 Radio Removal Tools

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the battery.
2. Remove the radio.

• | Install the removal bar KM6067 into the openings (arrows) until it engages.

• | Pull both removal bars outward and at the same time withdraw the radio from the holder.

3. Disconnect the wiring harness plug.

Disconnect the 2 wiring harness plugs (1, 2).

4. Remove the instrument panel (I/P) compartment.

• | Open the I/P compartment door.

• | Remove the 4 bolts (1).

• | Disconnect the wiring harness plug.

• | Remove the I/P compartment.

5. Remove the door sill inner panel.

• | Release the 5 clips.

• | Remove the door sill inner panel.

6. Lower the headlining. Refer to Headlining Trim Panel Replacement .
7. Remove the rear compartment side trim panel. Refer to Rear Compartment Side Trim Panel Replacement .
8. Disconnect the roof antenna wiring harness plug (1).
9. Disconnect the antenna cable (1) and insulate the remaining ends.

Important:

• | The old antenna cable remains in the wiring harness.

• | The new antenna cable is routed parallel to the existing antenna cable and is secured with duct tape and cable ties.

10. Route the antenna cable up to behind the I/P compartment.
11. Disconnect the antenna cable from the instrument panel padding wiring harness.

Disconnect and insulate the wiring harness (1).

### Installation Procedure

1. Connect the roof wiring harness.
2. Install the headlining. Refer to Headlining Trim Panel Replacement .
3. Install the radio.

• | Connect the 2 wiring harness plugs.

• | Radio must audibly engage.

4. Install the I/P compartment.

Connect the wiring harness plug.

Notice: Refer to Fastener Notice in the Preface section.

5. Install the I/P compartment.

Tighten
Tighten the 4 screws to 4 N·m (35 lb in).

6. Install the sill molding assembly.

Clip in the 5 clips.

7. Connect the battery.
8. For reprogramming procedures, refer to Control Module References .